C.4 Warning Status Class
Prev | C Status Type Encoding (Normative) | Next

## C.4 Warning Status Class

Statuses in this Status Class convey that the operation/notification has completed but an error was detected. The semantics and behavior of these Statuses are defined in PS3.4.

### C.4.1 Warning

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field is Service Class specific and defined in PS3.4.
Offending Element | (0000,0901) | AT | 1-n | This optional field contains a list of the elements in which the error was detected.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.

### C.4.2 Attribute List Error

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID for which Attributes were not recognized.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0107H.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field contains the UID of the SOP Instance for which Attributes were not recognized.
Attribute Identifier List | (0000,1005) | AT | 1-n | This optional field contains an Attribute Tag for each Attribute that was not recognized.

### C.4.3 Attribute Value Out of Range

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0116H.
Modification List/Attribute List | (no tag) | - | - | Optionally contains the application specific Data Set to only encode the invalid Attribute Values conveyed in the Modification List of the N-SET-RQ or the Attribute List of the N-CREATE-RQ.

Prev | Up | Next
C.3 Cancel Status Class | Home | C.5 Failure Status Class