C.5 Failure Status Class
Prev | C Status Type Encoding (Normative) | Next

## C.5 Failure Status Class

Statuses in this Status Class convey that the operation/notification failed and was not performed.

### C.5.1 Error: Cannot Understand

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field is Service Class specific and defined in PS3.4.
Offending Element | (0000,0901) | AT | 1-n | This optional field contains a list of the elements in which the error was detected.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.

### C.5.2 Error: Data Set Does Not Match SOP Class

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field is Service Class specific and defined in PS3.4.
Offending Element | (0000,0901) | AT | 1-n | This optional field contains a list of the elements in which the error was detected.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.

### C.5.3 Failed

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field is Service Class specific and defined in PS3.4.
Offending Element | (0000,0901) | AT | 1-n | This optional field contains a list of the elements in which the error was detected.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.

### C.5.4 Refused: Move Destination Unknown

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field is Service Class specific and defined in PS3.4.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.

### C.5.5 Refused: Out of Resources

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field is Service Class specific and defined in PS3.4.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.

### C.5.6 Refused: SOP Class Not Supported

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0122H.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.

### C.5.7 Class-Instance Conflict

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID for which the SOP Instance was not a member.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0119H.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field contains the SOP Instance that was not a member of the specified SOP Class.

### C.5.8 Duplicate SOP Instance

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0111H.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field contains the SOP Instance UID that was already allocated to another SOP Instance.

### C.5.9 Duplicate Invocation

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0210H.

### C.5.10 Invalid Argument Value

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0115H.
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID for which an argument value was in error.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field contains the ID of the SOP Instance for which an argument value was in error.
Event Type ID | (0000,1002) | US | 1 | This optional field contains the UID of the Event Type that was not recognized. Permitted only in the N-EVENT-RSP.
Event Information | (no tag) | - | - | Optionally contains the application specific Data Set to only encode the invalid argument values conveyed in the Event Information of the request. Permitted only in the N-EVENT-REPORT-RSP.
Action Type ID | (0000,1008) | US | 1 | This optional field contains the ID of the Action Type that was not recognized. Permitted only in the N-ACTION-RSP.
Action Information | (no tag) | - | - | Optionally contains the application specific Data Set to only encode the invalid argument values conveyed in the N-ACTION-RQ. Permitted only in the N-ACTION-RSP.

### C.5.11 Invalid Attribute Value

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0106H.
Modification List/Attribute List | (no tag) | - | - | Optionally contains the application specific Data Set to only encode the invalid Attribute Values conveyed in the Modification List of the N-SET -RQ or the Attribute List of the N-CREATE-RQ.

### C.5.12 Invalid Object Instance

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0117H.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field contains the SOP Instance UID that violated the UID construction rules.

### C.5.13 Missing Attribute

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0120H.
Attribute Identifier List | (0000,1005) | AT | 1-n | This optional field contains an Attribute Tag for each Attribute that was not recognized.

### C.5.14 Missing Attribute Value

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0121H.
Modification List/Attribute List | (no tag) | - | - | Optionally contains the application specific Data Set to only encode missing Attribute Values conveyed Modification List of the N-SET -RQ or the Attribute List of the N-CREATE-RQ..

### C.5.15 Mistyped Argument

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0212H.

### C.5.16 No Such Argument

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field shall optionally contain the SOP Class UID for which the argument does not exist.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0114H.
Event Type ID | (0000,1002) | US | 1 | This optional field contains the ID of the Event Type for which the argument does not exist. Permitted only in the N-EVENT-REPORT-RSP.
Action Type ID | (0000,1008) | US | 1 | This optional field contains the ID of the Action Type for which the argument does not exist. Permitted only in the N-ACTION-RSP.

### C.5.17 No Such Attribute

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0105H.
Attribute Identifier List | (0000,1005) | AT | 1-n | This optional field contains an Attribute Tag for each Attribute that was not recognized.

### C.5.18 No Such Event Type

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID for which the event type does not exist.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0113H.
Event Type ID | (0000,1002) | US | 1 | This optional field contains the ID of the Event Type that does not exist.

### C.5.19 No Such SOP Instance

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0112H.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field contains the SOP Instance UID that did not exist.

### C.5.20 No Such SOP Class

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID that does not exist.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0118H.

### C.5.21 Processing Failure

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID on which the processing failure occurred.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0110H.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.
Error ID | (0000,0903) | US | 1 | This optional field contains an application-specific error code.
Affected SOP Instance UID | (0000,1000) | UI | 1 | This optional field shall optionally contain the UID of the SOP Instance on which the processing failure occurred.

### C.5.22 Resource Limitation

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0213H.

### C.5.23 Unrecognized Operation

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0211H.

### C.5.24 No Such Action Type

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Affected SOP Class UID | (0000,0002) | UI | 1 | This optional field contains the SOP Class UID for which the action type does not exist.
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0123H.
Action Type ID | (0000,1008) | US | 1 | This optional field contains the ID of the Action Type that does not exist.

### C.5.25 Refused: Not Authorized

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0124H.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.

Prev | Up | Next
C.4 Warning Status Class | Home | D Association Negotiation (Normative)