7.2 Multi-frame and Video Image Objects
Prev | 7 Persistent Object Types | Next

## 7.2 Multi-frame and Video Image Objects

### 7.2.1 Objects Included

In this category are all SOP classes defined in PS3.3 that are multi-frame or video image objects.

### 7.2.2 MIME Type Constraints

The Server shall be able to send a response for the following MIME types:

- WADO-URI and WADO-WS

  - application/dicom

- WADO-RS

  - application/dicom

  - application/octet-stream

  - application/dicom+xml

  - application/json

If the contentType parameter is not present in the WADO-URI or WADO-WS request, the response shall contain a application/dicom MIME type.

The Server can optionally support the following MIME types for WADO-URI and WADO-WS:

- video/mpeg

- image/gif

The Server can optionally support the following MIME types for WADO-RS:

- image/dicom+jpx

- video/mpeg

- video/mp4

The Server may also support other MIME types.

Prev | Up | Next
7 Persistent Object Types | Home | 7.3 Text Objects