A.65 Ophthalmic Visual Field Static Perimetry Measurements IOD
Prev | A Composite Information Object Definitions (Normative) | Next

## A.65 Ophthalmic Visual Field Static Perimetry Measurements IOD

### A.65.1 Ophthalmic Visual Field Static Perimetry Measurements IOD Description

The Ophthalmic Visual Field Static Perimetry Measurements IOD is used to encode results of static perimetry with visual field devices.

### A.65.2 Ophthalmic Visual Field Static Perimetry Measurements IOD Entity-Relationship Model

The E-R Model in Section A.1.2 depicts those components of the DICOM Information Model that are referenced by the Ophthalmic Visual Field Static Perimetry Measurements IOD. Below the Series IE, only the Measurements IE is used.

### A.65.3 Ophthalmic Visual Field Static Perimetry Measurements IOD Modules

Table A.65.3-1 specifies the Modules of the Ophthalmic Visual Field Static Perimetry Measurements IOD.

Table A.65.3-1. Ophthalmic Visual Field Static Perimetry Measurements IOD Modules

IE | Module | Reference | Usage
--- | --- | --- | ---
Patient | Patient | C.7.1.1 | M
Clinical Trial Subject | C.7.1.3 | U
Study | General Study | C.7.2.1 | M
Patient Study | C.7.2.2 | U
Clinical Trial Study | C.7.2.3 | U
Series | General Series | C.7.3.1 | M
Clinical Trial Series | C.7.3.2 | U
Visual Field Static Perimetry Measurements Series | C.8.26.1 | M
Equipment | General Equipment | C.7.5.1 | M
Enhanced General Equipment | C.7.5.2 | M
Measurements | Visual Field Static Perimetry Test Parameters | C.8.26.2 | M
Visual Field Static Perimetry Test Reliability | C.8.26.3 | M
Visual Field Static Perimetry Test Measurements | C.8.26.4 | M
Visual Field Static Perimetry Test Results | C.8.26.5 | M
Ophthalmic Patient Clinical Information and Test Lens Parameters | C.8.26.6 | U
SOP Common | C.12.1 | M

Prev | Up | Next
A.64 RT Beams Delivery Instruction IOD | Home | A.66 Intravascular OCT IOD