CID 3680 ECG Lead Noise Descriptions
Prev | B DCMR Context Groups (Normative) | Next

## CID 3680 ECG Lead Noise Descriptions

This Context Group comprises the ECG noise annotations of ISO/IEEE 11073-10102. The terms included in the table below may not constitute the complete list; see the ISO/IEEE Standard.

### Note

Codes reprinted by permission of IEEE, Copyright 2004 by IEEE. ISO/IEEE 11073-10102 available through http://standards.ieee.org/.

Type:

  Extensible

Version:

  20110330

Table CID 3680. ECG Lead Noise Descriptions

Coding Scheme | Code Value | Code Meaning | ISO/IEEE 11073 MDC Equivalent Reference ID (Informative)
--- | --- | --- | ---
MDC | 10:11200 | No noise | MDC_ECG_NOISE_CLEAN
MDC | 10:11216 | Moderate noise | MDC_ECG_NOISE_MODERATE
MDC | 10:11232 | Severe noise | MDC_ECG_NOISE_SEVERE
MDC | 10:11248 | No signal | MDC_ECG_NOISE_NOSIGNAL

A prior version of this context group used codes from the SCP-ECG vocabulary.

Prev | Up | Next
CID 3679 ECG Morphology Descriptions (Retired) | Home | CID 3681 ECG Lead Noise Modifiers (Retired)