C.4 Spatial Calibration (SC) Class Requirements
Prev | C Ultrasound Application Profile (Normative) | Next

## C.4 Spatial Calibration (SC) Class Requirements

All implementations conforming to the Application Profile Class SC shall include the US Region Calibration Module with the exception of pixel component organization data element (0018,6044) and other data elements that are conditional on that data element.

Prev | Up | Next
C.3 General Class Profile | Home | C.5 Combined Calibration (CC) Class Requirements