B.27 RT Conventional Machine Verification Information Object Definition
Prev | B Normalized Information Object Definitions (Normative) | Next

## B.27 RT Conventional Machine Verification Information Object Definition

### B.27.1 IOD Description

The RT Conventional Machine Verification IOD describes the attributes that are required by an external Machine Parameter Verifier (MPV) when performing verification of a conventional (photon or electron) radiation therapy treatment, prior to delivery.

### B.27.2 IOD Modules

Table B.27.2-1. RT Conventional Machine Verification IOD Modules

Module | Reference | Module Description
--- | --- | ---
SOP Common | C.12.1 | Contains SOP Common Information
RT General Machine Verification | C.31.1 | Contains general delivery verification information
RT Conventional Machine Verification | C.31.2 | Contains delivery verification information specific to conventional (photon or electron) machines

Prev | Up | Next
B.26 Unified Procedure Step Information Object Definition | Home | B.28 RT Ion Machine Verification Information Object Definition