H.4.6.2.2 N-GET
Prev | H.4.6.2 DIMSE Service Group | Next

##### H.4.6.2.2 N-GET

The N-GET is used to retrieve an instance of the Printer SOP Class.

###### H.4.6.2.2.1 Attributes

The Attributes that may be retrieved are shown in Table H.4-17.

Table H.4-17. N-GET Attributes

Attribute Name | Tag | Usage SCU/SCP
--- | --- | ---
Printer Status | (2110,0010) | U/M
Printer Status Info | (2110,0020) | U/M
Printer Name | (2110,0030) | U/U
Manufacturer | (0008,0070) | U/U
Manufacturer Model Name | (0008,1090) | U/U
Device Serial Number | (0018,1000) | U/U
Software Versions | (0018,1020) | U/U
Date Last Calibration | (0018,1200) | U/U
Last Calibration | (0018,1201) | U/U

The meaning of the Usage SCU/SCP is described in Section H.2.4.

###### H.4.6.2.2.2 Behavior

The SCU uses the N-GET to request the SCP to get a Printer SOP Instance. The SCU shall specify in the N-GET request primitive the UID of the SOP Instance to be retrieved.

The SCP shall return the values for the specified Attributes of the specified SOP Instance.

The SCP shall return the status code of the requested SOP Instance retrieval. The meaning of success, warning, and failure status codes is defined in Section H.2.5.

Prev | Up | Next
H.4.6.2 DIMSE Service Group | Home | H.4.6.3 Printer Status Information