A.7.2.6 ReferencedFrames
Prev | A.7.2 Updated Pattern Based on A_DicomCompositeObjectReference Minimal (COCT_RM830120UV) | Next

#### A.7.2.6 ReferencedFrames

This act class shall be used if the referenced DICOM SOP instance is a multi-frame image and the reference does not apply to all frames. The list of integer values for the referenced frames of a DICOM multi-frame image SOP instance is contained in the Boundary ActClass.

Table A.7.2-4. DICOM Referenced Frames in an HL7 V3 Act

Attribute | Data Type | Multiplicity | Value
--- | --- | --- | ---
classCode | CS | 1..1 | ROIBND
moodCode | CS | 1..1 | EVN
templateId | LIST<II> | 1..* |
code | CV | 1..1 | < Code Value (0008,0100): 121190 as code property, 1.2.840.10008.2.16.4 as codeSystem property, DCM as codeSystemName property, Code Meaning (0008,0104): "Referenced Frames" as displayName property>

##### A.7.2.6.1 CDA Mapping (Class Name and Attributes used for CDA Documents)

- Act Clone Name: Observation

- Act clone name of the CDA entry is "Observation" instead of "ReferencedFrames"

- templateId value (Table A.7.1-4): Set root portion of II to "2.16.840.1.113883.10.20.6.2.10" (identifies the template that defines constraints on "Referenced Frames Observation" of CDA Diagnostic Imaging Reports as specified by CDA R2 DIR IG).

Prev | Up | Next
A.7.2.5 ActRelationship COMPONENT (SopInstance to ReferencedFrames) | Home | A.7.2.7 ActRelationship Component (ReferencedFrames to Boundary)