CID 3228 ECG Timing Measurements
Prev | B DCMR Context Groups (Normative) | Next

## CID 3228 ECG Timing Measurements

This Context Group include both global and per lead ECG measurements specified in the ISO/IEEE 11073-10102 MDC nomenclature. Note that the MDC codes for "per lead" measurements are base codes for post-coordination with separately encoded lead identifiers. MDC also defines pre-coordinated codes that include both the measurement and the lead, which may be used in the same context as this Context Group; see the ISO/IEEE Standard.

### Note

Codes reprinted by permission of IEEE, Copyright 2004 by IEEE. ISO/IEEE 11073-10102 available through http://standards.ieee.org/.

Type:

  Extensible

Version:

  20080927

Table CID 3228. ECG Timing Measurements

Coding Scheme Designator | Code Value | Code Meaning | ISO/IEEE 11073 MDC Equivalent Reference ID (Informative)
--- | --- | --- | ---
MDC | 2:15872 | PR interval global | MDC_ECG_TIME_PD_PR
MDC | 2:16160 | QT interval global | MDC_ECG_TIME_PD_QT
MDC | 2:16156 | QRS duration global | MDC_ECG_TIME_PD_QRS
MDC | 2:16184 | P duration global | MDC_ECG_TIME_PD_P
MDC | 2:16140 | PP interval global | MDC_ECG_TIME_PD_PP
MDC | 2:16168 | RR interval global | MDC_ECG_TIME_PD_RR
MDC | 2:7168 | PR interval per lead | MDC_ECG_TIME_PD_PR_<lead>
MDC | 2:8192 | QT interval per lead | MDC_ECG_TIME_PD_QT_<lead>
MDC | 2:7936 | QRS duration per lead | MDC_ECG_TIME_PD_QRS_<lead>
MDC | 2:6656 | P duration per lead | MDC_ECG_TIME_PD_P_<lead>
MDC | 2:32768 | PP interval per lead | MDC_ECG_TIME_PD_PP_<lead>
MDC | 2:33024 | RR interval per lead | MDC_ECG_TIME_PD_RR_<lead>

Prev | Up | Next
CID 3227 QTc Measurements | Home | CID 3229 ECG Axis Measurements