C.8.32.3 Parametric Map Functional Group Macros
Prev | C.8.32 Parametric Map | Next

#### C.8.32.3 Parametric Map Functional Group Macros

The following sections contain Functional Group Macros specific to the Parametric Map IOD.

### Note

The attribute descriptions in the Functional Group Macros are written as if they were applicable to a single frame (i.e., the macro is part of the Per-frame Functional Groups Sequence). If an attribute is applicable to all frames (i.e., the macro is part of the Shared Functional Groups Sequence) the phrase "this frame" in the attribute description shall be interpreted to mean "for all frames".

##### C.8.32.3.1 Parametric Map Frame Type Macro

Table C.8.32-3 specifies the attributes of the Parametric Map Frame Type Functional Group Macro.

Table C.8.32-3. Parametric Map Frame Type Macro Attributes

Attribute Name | Tag | Type | Attribute Description
--- | --- | --- | ---
Parametric Map Frame Type Sequence | (0040,9092) | 1 | Identifies the characteristics of this Parametric Map frame. Only a single Item shall be included in this sequence.
>Frame Type | (0008,9007) | 1 | Type of Frame. A multi-valued attribute analogous to Image Type (0008,0008). Enumerated Values and Defined Terms are the same as those for the four values of Image Type (0008,0008), except that the value MIXED is not allowed. See Section C.8.32.2.

Prev | Up | Next
C.8.32.2 Parametric Map Image Module | Home | C.9 Overlays