B.8 Annexes
Prev | B Conformance Statement Sample Integrated Modality (Informative) | Next

## B.8 Annexes

### B.8.1 IOD Contents

#### B.8.1.1 Created SOP Instances

Examples of X-Ray Radiofluoroscopic images and Grayscale Softcopy Presentation States created by EXAMPLE-INTEGRATED-MODALITY can be downloaded from:

http://www.example-imaging-products.nocom/example-integrated-modality/example-images

Table B.8.1-1 specifies the attributes of an X-Ray Radiofluoroscopic Image transmitted by the EXAMPLE-INTEGRATED-MODALITY storage application.

Table B.8.1-2 specifies the attributes of a Grayscale Softcopy Presentation State transmitted by the EXAMPLEINTEGRATED-MODALITY storage application.

The following tables use a number of abbreviations. The abbreviations used in the "Presence of …" column are:

VNAP

  Value Not Always Present (attribute sent zero length if no value is present)

ANAP

  Attribute Not Always Present

ALWAYS

  Always Present

EMPTY

  Attribute is sent without a value

The abbreviations used in the "Source" column:

MWL

  the attribute value source Modality Worklist

USER

  the attribute value source is from User input

AUTO

  the attribute value is generated automatically

MPPS

  the attribute value is the same as that use for Modality Performed Procedure Step

CONFIG

  the attribute value source is a configurable parameter

### Note

All dates and times are encoded in the local configured calendar and time. Date, Time and Time zone are configured using the Service/Installation Tool.

##### B.8.1.1.1 X-Ray Radiofluoroscopic Image IOD

Table B.8.1-1. IOD of Created Rf SOP Instances

IE | Module | Reference | Presence of Module
--- | --- | --- | ---
Patient | Patient | Table B.8.1-3 | ALWAYS
Study | General Study | Table B.8.1-4 | ALWAYS
Patient Study | Table B.8.1-5 | ALWAYS
Series | General Series | Table B.8.1-6 | ALWAYS
Equipment | General Equipment | Table B.8.1-7 | ALWAYS
Image | General Image | Table B.8.1-8 | ALWAYS
Image Pixel | Table B.8.1-10 | ALWAYS
Cine | Table B.8.1-11 | Only if Multi-frame
Multi-Frame | Table B.8.1-12 | Only if Multi-frame
Frame Pointers | Table B.8.1-13 | Only if Multi-frame
Mask | Table B.8.1-14 | ALWAYS
X-Ray Image | Table B.8.1-15 | ALWAYS
X-Ray Acquisition | Table B.8.1-16 | ALWAYS
Modality LUT | Table B.8.1-17 | Only if Pixel Intensity Relationship (0028,1040) is LOG
VOI LUT | Table B.8.1-18 | ALWAYS
SOP Common | Table B.8.1-19 | ALWAYS
Private Application | Table B.8.1-8 | ALWAYS

##### B.8.1.1.2 Grayscale Softcopy Presentation State IOD

Table B.8.1-2. IOD of Created Grayscale Softcopy Presentation State SOP Instances

IE | Module | Reference | Presence of Module
--- | --- | --- | ---
Patient | Patient | Table B.8.1-3 | ALWAYS
Study | General Study | Table B.8.1-4 | ALWAYS
Patient Study | Table B.8.1-5 | ALWAYS
Series | General Series | Table B.8.1-6 | ALWAYS
| Presentation Series | Table B.8.1-20 | ALWAYS
Equipment | General Equipment | Table B.8.1-7 | ALWAYS
Presentation State | Presentation State | Table B.8.1-21 | ALWAYS
Display Shutter | Table B.8.1-22 | Only if Shutter applied
Displayed Area | Table B.8.1-23 | ALWAYS
Graphic Annotation | Table B.8.1-24 | Only if Graphic Annotations are present
Spatial Transformation | Table B.8.1-25 | Only if Spacial Transformation applied
Graphic Layer | Table B.8.1-26 | Only if Graphic Annotations are present
Modality LUT | Table B.8.1-27 | ALWAYS
Softcopy VOI LUT | Table B.8.1-28 | ALWAYS
Softcopy Presentation LUT | Table B.8.1-29 | ALWAYS
SOP Common | Table B.8.1-19 | ALWAYS
Private Application | Table B.8.1-8 | ALWAYS

##### B.8.1.1.3 Common Modules

Table B.8.1-3. Patient Module of Created SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Patient's Name | (0010,0010) | PN | From Modality Worklist or user input. Values supplied via Modality Worklist will be entered as received. Values supplied via user input will contain all 5 components (some possibly empty). . Maximum 64 characters. | VNAP | MWL/USER
Patient ID | (0010,0020) | LO | From Modality Worklist or user input. Maximum 64 characters. | VNAP | MWL/USER
Patient's Birth Date | (0010,0030) | DA | From Modality Worklist or user input | VNAP | MWL/USER
Patient's Sex | (0010,0040) | CS | From Modality Worklist or user input | VNAP | MWL/USER
Patient Comments | (0010,4000) | LT | From User Input. Maximum 1024 characters. | VNAP | USER

Table B.8.1-4. General Study Module of Created SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Study Instance UID | (0020,000D) | UI | From Modality Worklist or generated by device | ALWAYS | MWL/AUTO
Study Date | (0008,0020) | DA | <yyyymmdd> | ALWAYS | AUTO
Study Time | (0008,0030) | TM | <hhmmss> | ALWAYS | AUTO
Referring Physician's Name | (0008,0090) | PN | From Modality Worklist | VNAP | MWL
Study ID | (0020,0010) | SH | Requested Procedure ID from Worklist or User Input | VNAP | MWL/USER
Accession Number | (0008,0050) | SH | From Modality Worklist or user input | VNAP | MWL/USER
Study Description | (0008,1030) | LO | Comment text box in study list. Maximum 1024 characters. | VNAP | USER
Referenced Study Sequence | (0008,1110) | SQ | From Modality Worklist | VNAP | MWL
>Referenced SOP Class UID | (0008,1150) | UI | From Modality Worklist | VNAP | MWL
>Referenced SOP Instance UID | (0008,1155) | UI | From Modality Worklist | VNAP | MWL

Table B.8.1-5. Patient Study Module of Created SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Admitting Diagnosis Description | (0008,1080) | LO | From Modality Worklist | VNAP | MWL
Patient's Age | (0010,1010) | AS | Calculated from DoB input on base of actual Date | ALWAYS | AUTO
Patient's Weight | (0010,1030) | DS | From Modality Worklist or user input | VNAP | MWL/USER

Table B.8.1-6. General Series Module of Created SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Modality | (0008,0060) | CS | RF | ALWAYS | AUTO
Series Instance UID | (0020,000E) | UI | Generated by device | ALWAYS | AUTO
Series Number | (0020,0011) | IS | Generated by device | ALWAYS | AUTO
Series Date | (0008,0021) | DA | <yyyymmdd> | ALWAYS | AUTO
Series Time | (0008,0031) | TM | <hhmmss> | ALWAYS | AUTO
Performing Physician's Name | (0008,1050) | PN | Physician field in Study list. Maximum 64 characters. | VNAP | USER
Protocol Name | (0018,1030) | LO | Organ program | ALWAYS | AUTO
Series Description | (0008,103E) | LO | Organ from Study list. Maximum 512 characters. | VNAP | USER
Operator's Name | (0008,1070) | PN | Operator field in Study list. Maximum 64 characters. | VNAP | USER
Referenced Performed Procedure Step Sequence | (0008,1111) | SQ | Identifies the MPPS SOP Instance to which this image is related | ALWAYS | MPPS
>Referenced SOP Class UID | (0008,1150) | UI | MPPS SOP Class UID | ALWAYS | MPPS
>Referenced SOP Instance UID | (0008,1155) | UI | MPPS SOP Instance UID | ALWAYS | MPPS
Request Attributes Sequence | (0040,0275) | SQ | Zero or 1 item will be present | ALWAYS | AUTO
>Requested Procedure ID | (0040,1001) | SH | From Modality Worklist | VNAP | MWL
>Scheduled Procedure Step ID | (0040,0009) | SH | From Modality Worklist | VNAP | MWL
>Scheduled Procedure Step Description | (0040,0007) | LO | From Modality Worklist | VNAP | MWL
>Scheduled Protocol Code Sequence | (0040,0008) | SQ | From Modality Worklist | VNAP | MWL
Performed Procedure Step ID | (0040,0253) | SH | Same as MPPS. | ALWAYS | MPPS
Performed Procedure Step Start Date | (0040,0244) | DA | Same as MPPS | ALWAYS | MPPS
Performed Procedure Step Start Time | (0040,0245) | TM | Same as MPPS | ALWAYS | MPPS
Performed Procedure Step Description | (0040,0254) | LO | Same as MPPS. From user input. Maximum 64 characters. | VNAP | MPPS
Performed Protocol Code Sequence | (0040,0260) | SQ | Same as MPPS | ALWAYS | MPPS
Comments on the Performed Procedure Step | (0040,0280) | LO | Same as MPPS. From user input. Maximum 64 characters. | VNAP | MPPS

Table B.8.1-7. General Equipment Module of Created SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Manufacturer | (0008,0070) | LO | EXAMPLE-IMAGING-PRODUCTS | ALWAYS | AUTO
Institution Name | (0008,0080) | LO | From Configuration | VNAP | CONFIG
Station Name | (0008,1010) | SH | From Configuration | ALWAYS | CONFIG
Manufacturer's Model Name | (0008,1090) | LO | EXAMPLE-INTEGRATED-MODALITY | ALWAYS | AUTO
Device Serial Number | (0018,1000) | LO | From Configuration | ALWAYS | CONFIG
Software Version | (0018,1020) | LO | From Configuration | ALWAYS | CONFIG
Private Creator | (0009,00xx) | LO | EXINTMOD_EQ_01 | ALWAYS | AUTO
Equipment UID | (0009,xx01) | UI | From Configuration | ALWAYS | CONFIG
Service UID | (0009,xx02) | UI | From Configuration | ALWAYS | CONFIG

Table B.8.1-8. Private Application Module of Created SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Private Creator | (0029,00xx) | LO | EXINTMOD_IM_01 | ALWAYS | AUTO
Application Header Sequence | (0029,xx40) | SQ | Zero or more items. Each item contains private application data from a different application. | VNAP | AUTO
>Private Creator | (0029,00xx) | LO | EXINTMOD_IM_01 | ALWAYS | AUTO
> Application Header Type | (0029,xx41) | CS | One of PLATFORM or PLUGIN | ALWAYS | AUTO
> Application Header ID | (0029,xx42) | LO | One of ACQUISITION, IMAGE PROCESSING, VIEWER, AUDIT, ACCESS, ROUTING or STATUS | ALWAYS | AUTO
> Application Header Version | (0029,xx43) | LO | From Application | ALWAYS | AUTO
> Application Header Data | (0029,xx44) | OB | From Application | ALWAYS | AUTO
Workflow Control Flags | (0029,xx50) | LO | One or more of:P: printedcom: completedrea: readver: verifiedRI: receivedAC: archived and committedE: exportedm: marked | VNAP | AUTO
Archive Management Flag - Keep Online | (0029,xx51) | CS | 00 = remote control not required (default)01 = keep instance online. | ALWAYS | AUTO
Archive Management Flag - Do Not Archive | (0029,xx52) | CS | 00 = remote control not required (default)01 = do not archive instance. | ALWAYS | AUTO

##### B.8.1.1.4 X-Ray Radiofluoroscopic Image Modules

Table B.8.1-9. General Image Module of Created Rf SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Instance Number | (0020,0013) | IS | Generated by device | ALWAYS | AUTO
Patient Orientation | (0020,0020) | CS | Zero length | EMPTY | AUTO
Content Date | (0008,0023) | DA | <yyyymmdd> | ALWAYS | AUTO
Content Time | (0008,0033) | TM | <hhmmss> | ALWAYS | AUTO
Acquisition Number | (0020,0012) | IS | Generated by device | ALWAYS | AUTO
Image Comments | (0020,4000) | LT | From user input. Maximum 1024 characters. | VNAP | USER
Anatomic Region Sequence | (0008,2218) | SQ | From user input. | ALWAYS | USER
> Include 'Code Sequence Macro' | Baseline Context ID is 4009 (see also Section B.8.6)

Table B.8.1-10. Image Pixel Module of Created Rf SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Pixel Data | (7FE0,0010) | OW | The Pixel Data itself does not contain any burned-in annotation. | ALWAYS | AUTO

Table B.8.1-11. Cine Module of Created Rf SOP

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Frame Time | (0018,1063) | DS | Only if multi-frame. | ANAP | AUTO
Recommended Display Frame Rate | (0008,2144) | IS | Only if multi-frame Same as Cine Rate | ANAP | AUTO
Cine Rate | (0018,0040) | IS | Only if multi-frame | ANAP | AUTO

Table B.8.1-12. Multi-Frame Module of Created Rf SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Number of Frames | (0028,0008) | IS | Only if multi-frame | ANAP | AUTO

Table B.8.1-13. Frame Pointers Module of Created Rf SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Representative Frame Number | (0028,6010) | US | Only if multi-frame | ANAP | AUTO

Table B.8.1-14. Mask Module of Created Rf SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Mask Subtraction Sequence | (0028,6100) | SQ | Only if multi-frame and (0028,1040) = LOG | ANAP | AUTO
> Mask Operation | (0028,6101) | CS | AVG_SUB | ANAP | AUTO
> Mask Frame Numbers | (0028,6110) | US | Mask Frame Number | ANAP | AUTO
Recommended Viewing Mode | (0028,1090) | CS | NAT or SUB | ALWAYS | AUTO

Table B.8.1-15. X-Ray Image Module of Created Rf SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Frame Increment Pointer | (0028,0009) | AT | <0018,1063> only if multi-frame | ANAP | AUTO
Image Type | (0008,0008) | CS | ORIGINAL\PRIMARY\SINGLE PLANE\DAS (acquired images) ORIGINAL\DERIVED\SINGLE PLANE (post-processed images) | ALWAYS | AUTO
Pixel Intensity Relationship | (0028,1040) | CS | LIN or LOG | ALWAYS | AUTO
Samples per Pixel | (0028,0002) | US | 1 | ALWAYS | AUTO
Photometric Interpretation | (0028,0004) | CS | MONOCHROME2 | ALWAYS | AUTO
Rows | (0028,0010) | US | 1024 | ALWAYS | AUTO
Columns | (0028,0011) | US | 1024 | ALWAYS | AUTO
Bits Allocated | (0028,0100) | US | 16 | ALWAYS | AUTO
Bits Stored | (0028,0101) | US | 10 | ALWAYS | AUTO
High Bit | (0028,0102) | US | 9 | ALWAYS | AUTO
Pixel Representation | (0028,0103) | US | 0000H | ALWAYS | AUTO

Table B.8.1-16. X-Ray Acquisition Module of Created Rf SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
KVP | (0018,0060) | DS | From Acquisition parameters | ALWAYS | AUTO
Radiation Setting | (0018,1155) | CS | GR | ALWAYS | AUTO
X-Ray Tube Current | (0018,1151) | IS | From Acquisition parameters | ALWAYS | AUTO
Exposure Time | (0018,1150) | IS | From Acquisition parameters | ALWAYS | AUTO
Radiation Mode | (0018,115A) | CS | CONTINUOUS | ALWAYS | AUTO
Intensifier Size | (0018,1162) | DS | From Acquisition parameters | ALWAYS | AUTO
Private Creator | (0019,00xx) | LO | EXINTMOD_AQ_01 | ALWAYS | AUTO
Edge Enhancement Percent | (0019,xx10) | IS | 0 .. 100 | VNAP | AUTO
Landmark | (0019,xx20) | IS | 0 .. 100 | VNAP | AUTO
Pixel Shift Horizontal | (0019,xx30) | DS | -20 .. +20 | VNAP | AUTO
Pixel Shift Vertical | (0019,xx40) | DS | -20 .. +20 | VNAP | AUTO

Table B.8.1-17. Modality LUT Module of Created Rf SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Modality LUT Sequence | (0028,3000) | SQ | present if (0028,1040) = LOG | ANAP | AUTO
> LUT Descriptor | (0028,3002) | US | <1024,0,16> | ANAP | AUTO
> Modality LUT Type | (0028,3004) | LO | US | ANAP | AUTO
> LUT Data | (0028,3006) | US | LUT | ANAP | AUTO

Table B.8.1-18. VOI LUT Module of Created Rf SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Window Center | (0028,1050) | DS | 0…1023 | ALWAYS | AUTO
Window Width | (0028,1051) | DS | 1…1024 | ALWAYS | AUTO

Table B.8.1-19. SOP Common Module of Created Rf SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Specific Character Set | (0008,0005) | CS | "ISO_IR 100" or "ISO_IR 144" | ALWAYS | CONFIG
SOP Class UID | (0008,0016) | UI | 1.2.840.10008.5.1.4.1.1.12.2 | ALWAYS | AUTO
SOP Instance UID | (0008,0018) | UI | Generated by device | ALWAYS | AUTO

##### B.8.1.1.5 Grayscale Softcopy Presentation State Modules

Table B.8.1-20. Presentation Series Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Modality | (0008,0060) | CS | PR | ALWAYS | AUTO

Table B.8.1-21. Presentation State Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Instance Number | (0020,0013) | IS | Generated by device | ALWAYS | AUTO
Presentation Label | (0070,0080) | CS | From user input. | ALWAYS | USER
Presentation Description | (0070,0081) | LO | From user input. | VNAP | USER
Presentation Creation Date | (0070,0082) | DA | Generated by device | ALWAYS | AUTO
Presentation Creation Time | (0070,0083) | TM | Generated by device | ALWAYS | AUTO
Presentation Creator's Name | (0070,0084) | PN | Generated by device according to currently active user. | ALWAYS | AUTO
Referenced Series Sequence | (0008,1115) | SQ | One or more items. | ALWAYS | AUTO
>Series Instance UID | (0020,000E) | UI | From referenced image | ALWAYS | AUTO
>Referenced Image Sequence | (0008,1140) | SQ | From referenced image | ALWAYS | AUTO
>>Referenced SOP Class UID | (0008,1150) | UI | From referenced image | ALWAYS | AUTO
>>Referenced SOP Instance UID | (0008,1155) | UI | From referenced image | ALWAYS | AUTO
>>Referenced Frame Number | (0008,1160) | IS | If referenced image is a multi-frame image | ANAP | AUTO
Shutter Presentation Value | (0018,1622) | US | Generated by device if shutter present | ANAP | AUTO

Table B.8.1-22. Display Shutter Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Shutter Shape | (0018,1600) | CS | If shutter applied: RECTANGULAR\CIRCULAR | ANAP | AUTO
Shutter Left Vertical Edge | (0018,1602) | IS | If RECTANGULAR shutter applied | ANAP | AUTO
Shutter Right Vertical Edge | (0018,1604) | IS | If RECTANGULAR shutter applied | ANAP | AUTO
Shutter Upper Horizontal Edge | (0018,1606) | IS | If RECTANGULAR shutter applied | ANAP | AUTO
Shutter Lower Horizontal Edge | (0018,1608) | IS | If RECTANGULAR shutter applied | ANAP | AUTO
Center of Circular Shutter | (0018,1610) | IS | If CIRCULAR shutter applied | ANAP | AUTO
Radius of Circular Shutter | (0018,1612) | IS | If CIRCULAR shutter applied | ANAP | AUTO

Table B.8.1-23. Displayed Area Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Displayed Area Selection Sequence | (0070,005A) | SQ | One or more items | ALWAYS | AUTO
>Referenced Image Sequence | (0008,1140) | SQ | One or more items | ALWAYS | AUTO
>>Referenced SOP Class UID | (0008,1150) | UI | From referenced image | ALWAYS | AUTO
>>Referenced SOP Instance UID | (0008,1155) | UI | From referenced image | ALWAYS | AUTO
>>Referenced Frame Number | (0008,1160) | IS | If referenced image is a multi-frame image | ANAP | AUTO
>Displayed Area Top Left Hand Corner | (0070,0052) | SL | From current display setting | ALWAYS | AUTO
>Displayed Area Bottom Right Hand Corner | (0070,0053) | SL | From current display setting | ALWAYS | AUTO
>Presentation Size Mode | (0070,0100) | CS | From current display setting | ALWAYS | AUTO
>Presentation Pixel Spacing | (0070,0101) | DS | From current display setting | ANAP | AUTO
>Presentation Pixel Aspect Ratio | (0070,0102) | IS | From current display setting | ANAP | AUTO
>Presentation Pixel Magnification Ratio | (0070,0103) | FL | From current display setting | ANAP | AUTO

Table B.8.1-24. Graphic Annotation Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Graphic Annotation Sequence | (0070,0001) | SQ | One or more items | ANAP | AUTO
>Referenced Image Sequence | (0008,1140) | SQ | One or more items | ALWAYS | AUTO
>>Referenced SOP Class UID | (0008,1150) | UI | From referenced image | ALWAYS | AUTO
>>Referenced SOP Instance UID | (0008,1155) | UI | From referenced image | ALWAYS | AUTO
>>Referenced Frame Number | (0008,1160) | IS | If referenced image is a multi-frame image | ANAP | AUTO
>Graphic Layer | (0070,0002) | CS | Layer in Graphic Layer Module | ALWAYS | AUTO
>Text Object Sequence | (0070,0008) | SQ | One or more items if text annotation present | ANAP | AUTO
>>Anchor Point Annotation Units | (0070,0004) | CS | PIXEL | ALWAYS | AUTO
>>Unformatted Text Value | (0070,0006) | ST | From user input | ALWAYS | USER
>>Anchor Point | (0070,0014) | FL | From user input | ALWAYS | USER
>>Anchor Point Visibility | (0070,0015) | CS | From user input | ALWAYS | USER
>Graphic Object Sequence | (0070,0009) | SQ | One or more items if graphic annotation present | ANAP | AUTO
>>Graphic Annotation Units | (0070,0005) | CS | PIXEL | ALWAYS | AUTO
>>Graphic Dimensions | (0070,0020) | US | 2 | ALWAYS | AUTO
>>Number of Graphic Points | (0070,0021) | US | From user input | ALWAYS | USER
>>Graphic Data | (0070,0022) | FL | From user input | ALWAYS | USER
>>Graphic Type | (0070,0023) | CS | One of POINT, POLYLINE, INTERPOLATED, CIRCLE or ELLIPSE | ALWAYS | USER
>>Graphic Filled | (0070,0024) | CS | From user input | ANAP | USER
Attribute Name | Tag | VR | Value | Presence of Value | Source
Graphic Annotation Sequence | (0070,0001) | SQ | One or more items | ANAP | AUTO
>Referenced Image Sequence | (0008,1140) | SQ | One or more items | ALWAYS | AUTO
>>Referenced SOP Class UID | (0008,1150) | UI | From referenced image | ALWAYS | AUTO
>>Referenced SOP Instance UID | (0008,1155) | UI | From referenced image | ALWAYS | AUTO
>>Referenced Frame Number | (0008,1160) | IS | If referenced image is a multi-frame image | ANAP | AUTO
>Graphic Layer | (0070,0002) | CS | Layer in Graphic Layer Module | ALWAYS | AUTO
>Text Object Sequence | (0070,0008) | SQ | One or more items if text annotation present | ANAP | AUTO
>>Anchor Point Annotation Units | (0070,0004) | CS | PIXEL | ALWAYS | AUTO
>>Unformatted Text Value | (0070,0006) | ST | From user input | ALWAYS | USER
>>Anchor Point | (0070,0014) | FL | From user input | ALWAYS | USER
>>Anchor Point Visibility | (0070,0015) | CS | From user input | ALWAYS | USER
>Graphic Object Sequence | (0070,0009) | SQ | One or more items if graphic annotation present | ANAP | AUTO
>>Graphic Annotation Units | (0070,0005) | CS | PIXEL | ALWAYS | AUTO
>>Graphic Dimensions | (0070,0020) | US | 2 | ALWAYS | AUTO
>>Number of Graphic Points | (0070,0021) | US | From user input | ALWAYS | USER
>>Graphic Data | (0070,0022) | FL | From user input | ALWAYS | USER
>>Graphic Type | (0070,0023) | CS | One of POINT, POLYLINE, INTERPOLATED, CIRCLE or ELLIPSE | ALWAYS | USER
>>Graphic Filled | (0070,0024) | CS | From user input | ANAP | USER

Table B.8.1-25. Spatial Transformation Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Image Rotation | (0070,0042) | US | From current display setting | ANAP | AUTO
Image Horizontal Flip | (0070,0041) | CS | From current display setting | ANAP | AUTO

Table B.8.1-26. Graphic Layer Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Graphic Layer Sequence | (0070,0060) | SQ | One or more items | ANAP | AUTO
>Graphic Layer | (0070,0002) | CS | LAYER1. LAYER2, LAYER3, … | ALWAYS | AUTO
>Graphic Layer Order | (0070,0062) | IS | From current display setting | ALWAYS | AUTO

Table B.8.1-27. Modality LUT Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Modality LUT Sequence | (0028,3000) | SQ | One item | ANAP | AUTO
>LUT Descriptor | (0028,3002) | US | <1024,0,16> | ALWAYS | AUTO
>Modality LUT Type | (0028,3004) | LO | US | ALWAYS | AUTO
>LUT Data | (0028,3006) | US | LUT | ALWAYS | AUTO
Rescale Intercept | (0028,1052) | DS | 1 | ANAP | AUTO
Rescale Slope | (0028,1053) | DS | 0 | ANAP | AUTO
Rescale Type | (0028,1054) | LO | US | ANAP | AUTO

Table B.8.1-28. Softcopy VOI LUT Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Softcopy VOI LUT Sequence | (0028,3110) | SQ | One or more items | ALWAYS | AUTO
>Referenced Image Sequence | (0008,1140) | SQ | One or more items | ALWAYS | AUTO
>>Referenced SOP Class UID | (0008,1150) | UI | From referenced image | ALWAYS | AUTO
>>Referenced SOP Instance UID | (0008,1155) | UI | From referenced image | ALWAYS | AUTO
>>Referenced Frame Number | (0008,1160) | IS | If referenced image is a multi-frame image | ANAP | AUTO
>Window Center | (0028,1050) | DS | From current display setting: 0…1023 | ALWAYS | AUTO
>Window Width | (0028,1051) | DS | From current display setting: 1…1024 | ALWAYS | AUTO
>Window Center & Width Explanation | (0028,1055) | LO | Name of Window Preset | ANAP | AUTO

Table B.8.1-29. Softcopy Presentation LUT Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Presentation LUT Shape | (2050,0020 | CS | IDENTITY | ALWAYS | AUTO

Table B.8.1-30. SOP Common Module of Created GSPS SOP Instances

Attribute Name | Tag | VR | Value | Presence of Value | Source
--- | --- | --- | --- | --- | ---
Specific Character Set | (0008,0005) | CS | "ISO_IR 100" or "ISO_IR 144" | ALWAYS | CONFIG
SOP Class UID | (0008,0016) | UI | 1.2.840.10008.5.1.4.1.1.11.1 | ALWAYS | AUTO
SOP Instance UID | (0008,0018) | UI | Generated by device | ALWAYS | AUTO

#### B.8.1.2 Used Fields in Received IOD By Application

The EXAMPLE-INTEGRATED-MODALITY storage application does not receive SOP Instances. The usage of attributes received via Modality Worklist is described in Section B.4.2.2.3.1.3.

#### B.8.1.3 Attribute Mapping

The relationships between attributes received via Modality Worklist, stored in acquired images and communicated via MPPS are summarized in Table B.8.1-31. The format and conventions used in DICOM Table B.8.1-31 are the same as the corresponding table in Section J.6 in PS3.17 .

Table B.8.1-31. Attribute Mapping Between Modality Worklist, Image and MPPS

Modality Worklist | Image IOD | MPPS IOD
--- | --- | ---
Patient Name | Patient Name | Patient Name
Patient ID | Patient ID | Patient ID
Patient's Birth Date | Patient's Birth Date | Patient's Birth Date
Patient's Sex | Patient's Sex | Patient's Sex
Patient's Weight | Patient's Weight |
Referring Physician's Name | Referring Physician's Name |
---- | ---- | Scheduled Step Attributes Sequence
Study Instance UID | Study Instance UID | >Study Instance UID
Referenced Study Sequence | Referenced Study Sequence | >Referenced Study Sequence
Accession Number | Accession Number | >Accession Number
---- | Request Attributes Sequence | ----
Requested Procedure ID | >Requested Procedure ID | >Requested Procedure ID
Requested Procedure Description |  | >Requested Procedure Description
Scheduled Procedure Step ID | >Scheduled Procedure Step ID | >Scheduled Procedure Step ID
Scheduled Procedure Step Description | >Scheduled Procedure Step Description | >Scheduled Procedure Step Description
Scheduled Protocol Code Sequence | >Scheduled Protocol Code Sequence | ----
---- | Performed Protocol Code Sequence | Performed Protocol Code Sequence
---- | Study ID | Study ID
---- | Performed Procedure Step ID | Performed Procedure Step ID
---- | Performed Procedure Step Start Date | Performed Procedure Step Start Date
---- | Performed Procedure Step Start Time | Performed Procedure Step Start Time
---- | Performed Procedure Step Description | Performed Procedure Step Description
---- | Comments on the Performed Procedure Step | Comments on the Performed Procedure Step
---- | ---- | Performed Series Sequence
Scheduled Performing Physician's Name | Performing Physician's Name | >Performing Physician's Name
Requested Procedure Code Sequence | ---- | Procedure Code Sequence
---- | Referenced Study Component Sequence | ----
---- | >Referenced SOP Class UID | SOP Class UID
---- | >Referenced SOP Instance UID | SOP Instance UID
---- | Protocol Name | Protocol Name

#### B.8.1.4 Coerced/Modified Fields

The Modality Worklist AE will truncate attribute values received in the response to a Modality Worklist Query if the value length is longer than the maximum length permitted by the attribute's VR.

Prev | Up | Next
B.7 Security | Home | B.8.2 Data Dictionary of Private Attributes