C.8.8.14.9 Compensator Thickness Data and Source to Compensator Distance
Prev | C.8.8.14 RT Beams Module | Next

##### C.8.8.14.9 Compensator Thickness Data and Source to Compensator Distance

The values stored in Compensator Thickness Data (300A,00EC) and Source to Compensator Distance (300A,02E2) shall be parallel to the radiation beam axis if Compensator Divergence (300A,02E0) equals ABSENT, or divergent according to the beam geometrical divergence if Compensator Divergence (300A,02E0) equals PRESENT. If Compensator Divergence (300A,02E0) is not sent, then the parallel or divergent nature of the thicknesses is as if ABSENT was specified for Compensator Divergence (300A,02E0).

Prev | Up | Next
C.8.8.14.8 Machine Rotations | Home | C.8.8.14.10 Compensator Transmission and Thickness Data Direction