D.8.4 Grayscale Image Consistency
Prev | D.8 Annexes | Next

### D.8.4 Grayscale Image Consistency

The high resolution display monitor attached to the product can be calibrated according to the Grayscale Standard Display Function (GSDF). The Service/Installation Tool is used together with a luminance meter to measure the Characteristic Curve of the display system and the current ambient light. See the product Service Manual for details on the calibration procedure and supported calibration hardware. The result of the calibration procedure is a Monitor Correction LUT that will be active within the display subsystem after a system reboot.

Prev | Up | Next
D.8.3 Coded Terminology and Templates | Home | D.8.5 Standard Extended/Specialized/Private SOP Classes