CID 6 Transducer Orientation
Prev | B DCMR Context Groups (Normative) | Next

## CID 6 Transducer Orientation

Type:

  Extensible

Version:

  20040322

Table CID 6. Transducer Orientation

Coding Scheme Designator | Code Value | Code Meaning
--- | --- | ---
SRT | G-A138 | Coronal
SRT | G-A143 | Longitudinal
SRT | G-A145 | Sagittal
SRT | G-A189 | Parasagittal
SRT | G-A472 | Oblique
SRT | G-A185 | Long axis
SRT | G-A13B | Off axis
SRT | G-A186 | Short axis
SRT | G-A191 | Five chamber
SRT | G-A19B | Two chamber
SRT | G-A19C | Four chamber
SRT | G-A117 | Transverse

### Note

In a prior version of this table, the code G-A11B was specified for the concept Parasagittal. The use of this code conflicts with its assignment to another concept in SNOMED, and its use in this context is deprecated. Although there is minimal possibility of misinterpretation with SOP Instances that may include the deprecated use, receiving applications should be aware of this change; see Annex J.

Prev | Up | Next
CID 5 Transducer Approach | Home | CID 7 Ultrasound Beam Path