TID 4011 Mammography CAD Density
Prev | Mammography CAD SR IOD Templates | Next

### TID 4011 Mammography CAD Density

This template provides the detail specific to a density.

Type:

  Non-Extensible

Order:

  Significant

Table TID 4011. Mammography CAD Density

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CODE | EV (111035, DCM, "Lesion Density") | 1 | MC | At least one of rows 1, 2, 3, 4, 5 shall be present | DCID 6008 “Density Modifier”
2 |  |  | CODE | EV (M-020F9, SRT, "Shape") | 1 | MC | At least one of rows 1, 2, 3, 4, 5 shall be present | DCID 6004 “Mammography Characteristics of Shape”
3 |  |  | CODE | EV (111037, DCM, "Margins") | 1-n | MC | At least one of rows 1, 2, 3, 4, 5 shall be present | DCID 6006 “Mammography Characteristics of Margin”
4 |  |  | INCLUDE | DTID 1400 “Linear Measurement” | 1-n | MC | At least one of rows 1, 2, 3, 4, 5 shall be present | If the measured path is encoded, the SCOORD and its by-reference relationship to the IMAGE in TID (1400) Linear Measurement shall be used.
5 |  |  | INCLUDE | DTID 1401 “Area Measurement” | 1-n | MC | At least one of rows 1, 2, 3, 4, 5 shall be present | If the measured path is encoded, the SCOORD and its by-reference relationship to the IMAGE in TID (1401) Area Measurement shall be used.
6 |  |  | INCLUDE | DTID 1402 “Volume Measurement” | 1-n | U |  | If the measured path is encoded, the SCOORD and its by-reference relationship to the IMAGE in TID (1402) Volume Measurement shall be used.

Prev | Up | Next
TID 4010 Mammography CAD Calcification Cluster | Home | TID 4012 Mammography CAD Non-Lesion