8.2.10 Unique Identifier of the Series Containing The Presentation Object
Prev | 8.2.1 Annotation On The Object | Next

### 8.2.10 Unique Identifier of the Series Containing The Presentation Object

The parameter name shall be "presentationSeriesUID" for URI based mode, and "PresentationSeriesUID" for the WS mode.

Series Instance UID of the series containing the presentation state storage object to be applied on the images. This parameter is REQUIRED and shall only be present if "presentationUID" is present.

The value shall be encoded as a unique identifier (UID) string, as specified in PS3.5, except that it shall not be padded to an even length with a NULL character.

### Note

As specified in DICOM, the Presentation State will be in the same study as the images it applies to.

Prev | Up | Next
8.2.9 Unique Identifier of the Presentation Object | Home | 8.2.11 Transfer Syntax UID