A.27.3 Overlay Plane Module
Prev | A.27 Digital Mammography X-Ray Image IOD | Next

### A.27.3 Overlay Plane Module

If the Overlay Plane Module is present, any Overlays defined in that Module shall store the overlay data in Overlay Data (60xx,3000), and not any unused high bits in Pixel Data (7FE0,0010).

Prev | Up | Next
A.27.2 Digital Mammography X-Ray Image IOD Module Table | Home | A.28 Digital Intra-Oral X-Ray Image IOD