6.5.3.2.2 Bulk Data Response
Prev | 6.5.3.2 Response | Next

##### 6.5.3.2.2 Bulk Data Response

- Content-Type:

  - multipart/related; type=application/octet-stream; boundary={MessageBoundary}

  - multipart/related; type={MediaType}; boundary={MessageBoundary}

- The entire multipart response contains all bulk data for the specified Instance that can be converted to one of the requested media types.

- Each item in the response is one of:

  - an uncompressed bulk data element encoded in Little Endian binary format with the following headers:

    - Content-Type: application/octet-stream

    - Content-Location: {BulkDataURL}

  - a compressed bulk data element from a SOP Instance encoded in a single-frame media type with the following headers:

    - Content-Type: {MediaType}

    - Content-Location: {BulkDataURL}

  - a compressed frame from a multi-frame SOP Instance encoded in a single-frame media type with the following headers:

    - Content-Type: {MediaType}

    - Content-Location: {BulkDataURL}/frames/{FrameNumber}

  - a set of compressed frames from a multi-frame SOP Instance encoded in a multi-frame media type with the following headers:

    - Content-Type: {MediaType}

    - Content-Location: {BulkDataURL}[/frames/{FrameList}]

      - {FrameList} is a list of frames separated by %2C (comma). It may be omitted if the message part includes all frames for the specified bulk pixel data object.

Prev | Up | Next
6.5.3.2 Response | Home | 6.5.4 WADO-RS - RetrieveFrames