B.4 TID 2006 "Imaging Report with Conditional Radiation Exposure and Protection Information" Specific Mapping Requirements
Prev | B Imaging Report with Conditional Radiation Exposure and Protection Information Transformation Guide |

## B.4 TID 2006 "Imaging Report with Conditional Radiation Exposure and Protection Information" Specific Mapping Requirements

In addition to the transformations listed in Section B.3, TID 2006-specific contents shall be mapped as outlined below.

Study Date and Study Time in TID 2007 Imaging Procedure Description:

The study date and time observation is modeled as a CDA section component and shall be encoded as a section entry.

Table B.4-1. Study Date and Time Observation

Attribute | Data Type | Multiplicity | Value
--- | --- | --- | ---
classCode | CS | 1..1 | OBS
moodCode | CS | 1..1 | EVN
code | CE | 1..1 | <"113014" as code property,"1.2.840.10008.2.16.4"as codeSystem property,"DCM"as codeSystemName property, "Study" as displayName property>
effectiveTime | TS | 1..1 | "Study Date" value (DATE Value Type) and if present "Study Time" value (TIME Value Type)
languageCode | CE | 0..1 | Not used at entry level.
value | ANY | 0..1 | Not used.

The syntax of Point in Time (TS) is "YYYYMMDDHHMMSS.UUUU[+|-ZZzz]" where digits can be omitted from the right side to express less precision. If only "Study Date" is available from TID 2007, the form "YYYYMMDD" can be used.

Reference to Composite Objects in TID 2007 Imaging Procedure Description:

References to Composite Objects are used for DICOM objects that are not DICOM Images or Waveforms, for instance to SR Documents or to HL7 Structured Documents. Composite object reference observations are modeled as CDA section components and shall be encoded as section entries. The mapping of SopInstance references for composite objects is identical to image SopInstance references (please refer to PS 3.20 Annex A SR Diagnostic Imaging Report Transformation Guide for detailed information).

Figure B.4-1. Composite Object References

Table B.4-2. Composite Object Reference Observation

Attribute | Data Type | Multiplicity | Value
--- | --- | --- | ---
classCode | CS | 1..1 | OBS
moodCode | CS | 1..1 | EVN
templateId | LIST<II> | 1..* |
code | CE | 0..1 | Concept Name Code Sequence (0040,A043) of COMPOSITE Content Item (required if the Purpose of Reference is conveyed in the Concept Name): <code value as code property, coding scheme designator as codeSystemName property, code meaning as displayName property>
effectiveTime | TS | 0..1 | Not used.
languageCode | CE | 0..1 | Not used at entry level.
value | ANY | 0..1 | Not used.

The following Observation.code values shall be used for TID 2007 references to DICOM SR X-Ray Radiation Dose Reports: <"113701" as code property,"1.2.840.10008.2.16.4"as codeSystem property,"DCM"as codeSystemName property, "X-Ray Radiation Dose Report" as displayName property>.

"Irradiation Authorizing" (Value Type PNAME) in TID 2008 Radiation Exposure and Protection Information

The attributes of the "Irradiation Authorizing" PNAME content item are mapped to the ServiceEvent performer participation associated role and entities as specified in Table B.4-3, Table B.4-2 and Table B.4-5.

Figure B.4-2. Irradiation Authorizing Service Event Participation

Table B.4-3. Performer Participation

Attribute | Data Type | Multiplicity | Value
--- | --- | --- | ---
typeCode | CS | 1..1 | PRF
functionCode | CE | 0..1 | Shall not be sent.
time | IVL<TS> | 0..1 | Shall not be sent.

Table B.4-4. Assigned Entity

Attribute | Data Type | Multiplicity | Value
--- | --- | --- | ---
classCode | CS | 1..1 | ASSIGNED
id | SET<II> | 1..* | Use null flavor value "NI" (No Information) if the value cannot be obtained from some other source.
code | CE | 1..1 | Concept Name Code Sequence (0040,A043) of PNAME Content Item: <"113850" as code property, "1.2.840.10008.2.16.4" as codeSystem property, "DCM" as codeSystemName property, "Irradiation Authorizing" as displayName property>.
addr | SET<AD> | 0..* | Shall not be sent.
telecom | SET<TEL> | 0..* | Shall not be sent.

Table B.4-5. Person

Attribute | Data Type | Multiplicity | Value
--- | --- | --- | ---
classCode | CS | 1..1 | PSN
determinerCode | CS | 1..1 | INSTANCE
name | PN | 1..1 | Person Name (0040,A123)

Prev | Up |
B.3 HL7 CDA Release 2 Diagnostic Imaging Report Target Structure | Home |