S.2.3 LDAP Server
Prev | S.2 Managed Association Requester, Legacy Association Acceptor | Next

### S.2.3 LDAP Server

The LDAP server should be configured with a full description of the legacy Association Acceptor, even though the Association Acceptor itself cannot provide this information. This will need to be done manually, most likely using GUI tools. The legacy Association Acceptor will need to be manually configured to match the EYE-Titles and other configuration information.

Prev | Up | Next
S.2.2 DNS Server | Home | S.3 No DDNS Support