C.8.8.14.6 Absolute and Relative Machine Coordinates
Prev | C.8.8.14 RT Beams Module | Next

##### C.8.8.14.6 Absolute and Relative Machine Coordinates

All treatment machine parameters except couch translations are specified in absolute machine coordinates as defined by IEC 61217. For the Table Top Vertical Position (300A,0128), Table Top Longitudinal Position (300A,0129), and Table Top Lateral Position (300A,012A), if the first Control Point contains a value of non-zero length, all subsequent Control Point position values are absolute values in their respective coordinate system. If the first Control Point contains a zero-length value, all subsequent Control Point position values are specified relative to the (unknown) initial value.

Prev | Up | Next
C.8.8.14.5 Control Point Sequence | Home | C.8.8.14.7 Cumulative Dose Reference Coefficient