C.8.8.3.4 Image Pixel Module Attributes
Prev | C.8.8.3 RT Dose Module | Next

##### C.8.8.3.4 Image Pixel Module Attributes

###### C.8.8.3.4.1 Samples Per Pixel

Enumerated Values:

1

###### C.8.8.3.4.2 Photometric Interpretation

Enumerated Values:

MONOCHROME2

###### C.8.8.3.4.3 Bits Allocated

Enumerated Values:

16

32

###### C.8.8.3.4.4 Bits Stored

For RT Doses, Bits Stored (0028,0101) shall be equal to Bits Allocated (0028,0100).

###### C.8.8.3.4.5 High Bit

For RT Doses, High Bit (0028,0102) shall be one less than the value sent in Bits Stored (0028,0101).

###### C.8.8.3.4.6 Pixel Representation

Enumerated Values when Dose Type (3004,0004) = ERROR:

0001H

  two's complement integer,

Enumerated Values when Dose Type (3004,0004) not ERROR:

0000H

  unsigned integer, otherwise.

Prev | Up | Next
C.8.8.3.3 Dose Units | Home | C.8.8.3.5 Referenced Spatial Registration Sequence