V.3.3 Hanging Protocol Display Module
Prev | V.3 Chest X-Ray Hanging Protocol Example | Next

### V.3.3 Hanging Protocol Display Module

- Display Sets Sequence:

  - Item 1:

    - Display Set Number: 1

    - Display Set Presentation Group: 1

    - Image Set Number: 2

    - Image Boxes Sequence:

      - Item 1:

        - Image Box Number: 1

        - Display Environment Spatial Position: 0.0\1.0\0.25\0.0, representing (0,1), (0.25,0)

        - Image Box Layout Type: "SINGLE"

    - Filter Operations Sequence:

      - o Item 1:

        - Selector Attribute: (0018,5101) [View Position]

        - Selector Attribute VR: "CS"

        - Selector CS Value: "RL\LL"

        - Selector Value Number: 1

        - Filter-by Operator: "MEMBER_OF"

    - Sorting Operations Sequence: zero length

    - Display Set Patient Orientation: "A\F"

    - Show Image True Size Flag: "NO"

    - Show Graphic Annotation Flag: "NO"

  - Item 2:

    - Display Set Number: 2

    - Display Set Presentation Group: 1

    - Image Set Number: 2

    - Image Boxes Sequence:

      - Item 1:

        - Image Box Number: 1

        - Display Environment Spatial Position: 0.25\1.0\0.5\0.0, representing (0.25,1), (0.5,0)

        - Image Box Layout Type: "SINGLE"

    - Filter Operations Sequence:

      - Item 1:

        - Selector Attribute: (0018,5101) [View Position]

        - Selector Attribute VR: "CS"

        - Selector CS Value: "PA"

        - Selector Value Number: 1

        - Filter-by Operator: "MEMBER_OF"

    - Sorting Operations Sequence: zero length

    - Display Set Patient Orientation: "R\F"

    - Show Image True Size Flag: "NO"

    - Show Graphic Annotation Flag: "NO"

  - Item 3:

    - Display Set Number: 3

    - Display Set Presentation Group: 1

    - Image Set Number: 1

    - Image Boxes Sequence:

      - Item 1:

        - Image Box Number: 1

        - Display Environment Spatial Position: 0.5\1.0\0.75\1.0, representing (0.5,1), (0.75,0)

        - Image Box Layout Type: "SINGLE"

    - Filter Operations Sequence:

      - Item 1:

        - Selector Attribute: (0018,5101) [View Position]

        - Selector Attribute VR: "CS"

        - Selector CS Value: "PA"

        - Selector Value Number: 1

        - Filter-by Operator: "MEMBER_OF"

    - Sorting Operations Sequence: zero length

    - Display Set Patient Orientation: "R\F"

    - Show Image True Size Flag: "NO"

    - Show Graphic Annotation Flag: "NO"

  - Item 4:

    - Display Set Number: 4

    - Display Set Presentation Group: 1

    - Image Set Number: 1

    - Image Boxes Sequence:

      - Item 1:

        - Image Box Number: 1

        - Display Environment Spatial Position: 0.75\1.0\1.0\0.0, representing (0.75,1), (1,0)

        - Image Box Layout Type: "SINGLE"

    - Filter Operations Sequence:

      - Item 1:

        - Selector Attribute: (0018,5101) [View Position]

        - Selector Attribute VR: "CS"

        - Selector CS Value: "RL\LL"

        - Selector Value Number: 1

        - Filter-by Operator: "MEMBER_OF"

    - Sorting Operations Sequence: zero length

    - Display Set Patient Orientation: "A\F"

    - Show Image True Size Flag: "NO"

    - Show Graphic Annotation Flag: "NO"

- Partial Data Display Handling: "MAINTAIN_LAYOUT"

Prev | Up | Next
V.3.2 Hanging Protocol Environment Module | Home | V.4 Neurosurgery Planning Hanging Protocol Example