A.48.2 Enhanced XRF Image IOD Entity-Relationship Model
Prev | A.48 Enhanced X-Ray RF Image IOD | Next

### A.48.2 Enhanced XRF Image IOD Entity-Relationship Model

The E-R Model in Section A.1.2 depicts those components of the DICOM Application Information Model that directly reference the X-Ray RF Image IOD. Additionally, "Image" in Figure A.1-1 may represent a single frame or a multi-frame image. A frame denotes a two-dimensional organization of pixels recorded as a single exposure.

Prev | Up | Next
A.48 Enhanced X-Ray RF Image IOD | Home | A.48.3 Enhanced XRF Image IOD Module Table