PS3.8
|  | Next

# PS3.8

## DICOM PS3.8 2015a - Network Communication Support for Message Exchange

### DICOM Standards Committee

Copyright © 2015 NEMA

List of Figures

1-1. ISO OSI Basic Reference Model
6-1. DICOM Network Protocol Architecture
7-1. Associate Request
7-2. Association Release
7-3. Association User Initiated Abort
7-4. Provider Initiated Abort
7-5. Data Transfer
9-1. Protocol Data Units Structure and Encoding
9-2. Protocol Data Units Structure and Encoding
E.2-1. Presentation Data Value and the Message Control Header
G-1. Relationship of Services to Protocol
G-2. Service Description Conventions

List of Tables

7-1. Upper Layer Services
7-2. Key A-ASSOCIATE Service Parameters
7-3. A-ASSOCIATE Service Parameter (Fixed or Not Used)
7-4. A-RELEASE Service Parameters
7-5. A-ABORT Service Parameters
7-6. A-P-ABORT Service Parameters
7-7. P-DATA Service Parameter
9-1. No Association
9-2. Association Establishment
9-3. Data Transfer
9-4. Association Release
9-5. Waiting for Transport Connection Close
9-6. Association Establishment Related Actions
9-7. Data Transfer Related Actions
9-8. Association Release Related Actions
9-9. Association Abort Related Actions
9-10. DICOM Upper Layer Protocol State Transition Table
9-11. ASSOCIATE-RQ PDU Fields
9-12. Application Context Item Fields
9-13. Presentation Context Item Fields
9-14. Abstract Syntax Sub-Item Fields
9-15. Transfer Syntax Sub-Item Fields
9-16. User Information Item Fields
9-17. ASSOCIATE-AC PDU Fields
9-18. Presentation Context Item Fields
9-19. Transfer Syntax Sub-Item Fields
9-20. User Information Item Fields
9-21. ASSOCIATE-RJ PDU Fields
9-22. P-DATA-TF PDU Fields
9-23. Presentation-Data-Value Item Fields
9-24. A-RELEASE-RQ PDU Fields
9-25. A-RELEASE-RP PDU Fields
9-26. A-ABORT PDU Fields
D.1-1. Maximum Length Sub-Item Fields (A-ASSOCIATE-RQ)
D.1-2. Maximum Length Sub-Item Fields (A-ASSOCIATE-AC)

|  | Next
|  | Notice and Disclaimer