7.5 Sequencing Information
Prev | 7 OSI Upper Layer Service for DICOM Application Entities | Next

## 7.5 Sequencing Information

Interactions among the specific service procedures, discussed in Section 7.1, Section 7.2, Section 7.3 and Section 7.4 for the ACSE subset of the Upper Layer Service, are defined in clause 10 of ISO 8649 - The ACSE Service Definition.

Prev | Up | Next
7.4.2 A-P-ABORT Service Procedure | Home | 7.6 P-DATA Service