E.2 Retired Command Fields
Prev | E Command Dictionary (Normative) | Next

## E.2 Retired Command Fields

The following command fields have been retired but are listed here for compatibility with previous versions of this Standard. Reference PS3.5 for more information on retired Data Elements and Command Elements.

Table E.2-1. Retired Command Fields

Tag | Message Field | Keyword | VR | VM
--- | --- | --- | --- | ---
(0000,0001) | Command Length to End | CommandLengthToEnd | UL | 1
(0000,0010) | Command Recognition Code | CommandRecognitionCode | SH | 1
(0000,0200) | Initiator | Initiator | AE | 1
(0000,0300) | Receiver | Receiver | AE | 1
(0000,0400) | Find Location | FindLocation | AE | 1
(0000,0850) | Number of Matches | NumberOfMatches | US | 1
(0000,0860) | Response Sequence Number | ResponseSequenceNumber | US | 1
(0000,4000) | Dialog Receiver | DialogReceiver | LT | 1
(0000,4010) | Terminal Type | TerminalType | LT | 1
(0000,5010) | Message Set ID | MessageSetID | SH | 1
(0000,5020) | End Message ID | EndMessageID | SH | 1
(0000,5110) | Display Format | DisplayFormat | LT | 1
(0000,5120) | Page Position ID | PagePositionID | LT | 1
(0000,5130) | Text Format ID | TextFormatID | CS | 1
(0000,5140) | Normal/Reverse | NormalReverse | CS | 1
(0000,5150) | Add Gray Scale | AddGrayScale | CS | 1
(0000,5160) | Borders | Borders | CS | 1
(0000,5170) | Copies | Copies | IS | 1
(0000,5180) | Command Magnification Type | CommandMagnificationType | CS | 1
(0000,5190) | Erase | Erase | CS | 1
(0000,51A0) | Print | Print | CS | 1
(0000,51B0) | Overlays | Overlays | US | 1-n

### Note

For attributes that were present in ACR-NEMA 1.0 and 2.0 and that have been retired, the specifications of Value Representation and Value Multiplicity provided are recommendations for the purpose of interpreting their values in objects created in accordance with earlier versions of this standard. These recommendations are suggested as most appropriate for a particular attribute; however, there is no guarantee that historical objects will not violate some requirements or specified VR and/or VM.

Prev | Up | Next
E Command Dictionary (Normative) | Home | F Usage of the P-DATA Service By the DICOM Application Entity (Normative)