C Status Type Encoding (Normative)
Prev |  | Next

# C Status Type Encoding (Normative)

The following sections define the encoding for the Status Types supported by the DIMSE services. The semantics for each Status Type (i.e., Attribute List Error, etc.) are defined in the DIMSE Services. Each Status Type is categorized in a Status Class.

### Note

The Status (0000,0900) Command Element is required for all Status Types.

All Status Codes are assigned according to the following Status Class convention:

Success | 0000
Warning | 0001 or Bxxx
Failure | Axxx or Cxxx
Cancel | FE00
Pending | FF00 and FF01
PS3.7 Annex C assigned Warning and Failure | 01xx and 02xx

## C.1 Success Status Class

Statuses in this Status Class convey that the operation/notification completed successfully.

### C.1.1 Success

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field shall be set to 0000H.

Prev |  | Next
B Index to Application Context Name UIDs (Informative) | Home | C.2 Pending Status Class