TID 3317 Stress Imaging Summary
Prev | Stress Testing Report Templates | Next

### TID 3317 Stress Imaging Summary

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 3317. Stress Imaging Summary

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CODE | DT (122739, DCM, "Overall study quality") | 1 | M |  | BCID 3114 “Study Quality”
2 |  |  | CODE | DT (113010, DCM, "Quality Issue") | 1 | U |  | BCID 3115 “Stress Imaging Quality Issues”
3 |  |  | CODE | EV (121071, DCM, "Finding") | 1 | U |  | BCID 3116 “NM Extracardiac Findings”
4 |  |  | INCLUDE | DTID 300 “Measurement” | 1-2 | U |  | $Measurement = DT (F-04F76, SRT, "Perfusion defect extent") $ModType = EV (109054, DCM, "Patient State") $ModValue = DCID 3102 “Rest-Stress” $Units = EV (%, UCUM, "%") See note.
5 |  |  | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DT (F-04FCD, SRT, "Stress ischemia extent") $Units = EV (%, UCUM, "%")
6 |  |  | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DT (122762, DCM, "Number of diseased vessel territories") $Units = EV ({territories}, UCUM, "territories")
7 |  |  | CODE | EV (121071, DCM, "Finding") | 1 | U |  | EV (D3-13040, SRT, "Coronary artery disease")
8 | > | HAS PROPERTIES | CODE | EV (G-C0E3, SRT, "Finding Site") | 1-n | M |  | BCID 3016 “Major Coronary Arteries”
9 |  |  | CODE | EV (F-0238D, SRT, "Myocardial perfusion") | 1-2 | U |  | BCID 3120 “Perfusion Findings”
10 | > | HAS CONCEPT MOD | CODE | EV (G-C0E3, SRT, "Finding Site") | 1 | M |  | BCID 3463 “Ventricle Identification”
11 | > | HAS PROPERTIES | CODE | EV (G-C504, SRT, "Associated Morphology") | 1 | U |  | BCID 3121 “Perfusion Morphology”
12 |  |  | CODE | EV (121071, DCM, "Finding") | 1 | U |  | DT (D4-31124, SRT, "Transient cavitary dilatation")
13 | > |  | INCLUDE | DTID 1350 “Negation Modifier, Presence of Finding” | 1 | U |  |
14 |  |  | INCLUDE | DTID 300 “Measurement” | 1 | U |  | $Measurement = DT (F-04FB4, SRT, "Transient cavitary dilatation ratio") $Units = EV ({ratio}, UCUM, "ratio")
15 |  |  | INCLUDE | DTID 300 “Measurement” | 1-2 | U |  | $Measurement = EV (10230-1, LN, "LV Ejection Fraction") $ModType = EV (109054, DCM, "Patient State") $ModValue = DCID 3102 “Rest-Stress” $Units = EV (%, UCUM, "%") See note.

Content Item Descriptions

Row 4 | This row may be instantiated twice, once for resting state measurements, once for stress.
Row 15 | The LVEF code specified in this row is defined in LOINC with method "imaging". LVEF measurement by ultrasound may also be encoded elsewhere in the Content Tree (e.g., in TID 3309 “Stress Echo Measurement Group”) with LOINC code 18043-0, which has method "ultrasound". It is recommended that such findings from the per-phase measurements be summarized here with the generic "LVEF by Imaging" concept code.

Prev | Up | Next
TID 3313 Stress ECG Summary | Home | TID 3318 Comparison to Prior Stress Exam