TID 4023 CAD Operating Points
Prev | Mammography CAD SR IOD Templates | Next

### TID 4023 CAD Operating Points

This Template describes CAD operating points. The description is deliberately left flexible and optional to allow implementation at differing levels of complexity.

Type:

  Non-Extensible

Order:

  Significant

Root:

  No

Table TID 4023. CAD Operating Points

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  | HAS PROPERTIES | NUM | EV (111072, DCM, "Maximum CAD Operating Point") | 1 | M |  | UNITS = DT ([arb'U], UCUM, "arbitrary unit") Value is restricted to being an integer
2 |  | HAS PROPERTIES | NUM | EV (111092, DCM, "Recommended CAD Operating Point") | 1 | U |  | UNITS = DT ({0:n}, UCUM, "range: 0:n"), where n is the value specified in row 1 Value is restricted to being an integer
3 |  | HAS PROPERTIES | CONTAINER | EV (111093, DCM, "CAD Operating Point Table") | 1 | U |  |
4 | > | CONTAINS | CODE | EV (122698, DCM, "X-Concept") | 1 | M |  | DCID 6048 “CAD Operating Point Axis Label”
5 | > | CONTAINS | CODE | EV (122699, DCM, "Y-Concept") | 1 | M |  | DCID 6048 “CAD Operating Point Axis Label”
6 | > | CONTAINS | NUM | EV (111071, DCM, "CAD Operating Point") | 1-n | M | Number of instances of this row shall equal value of row 1, plus 1. | UNITS = DT ({0:n}, UCUM, "range: 0:n"), where n is the value of Row 1. Value is restricted to being an integer that is unique within the invocation of this Template.
7 | >> | HAS PROPERTIES | TEXT | EV (111081, DCM, "CAD Operating Point Description") | 1 | U |  |
8 | >> | HAS PROPERTIES | NUM | The value of Row 4 | 1 | U |  |
9 | >> | HAS PROPERTIES | NUM | The value of Row 5 | 1 | U |  |

Content Item Descriptions

Maximum CAD Operating Point | The maximum possible value of CAD Operating Point for this type of Detection Performed. No CAD Operating Point value recorded in the CAD Processing and Findings Summary sub-tree of the report for this type of Detection Performed shall exceed this value. The report may or may not contain Rendering Intent = "Presentation Optional" detections that are assigned the maximum value.
Recommended CAD Operating Point | A number indicating which of the CAD operating points is recommended by the creator of a CAD SR instance as the first operating point to be used when rendering the CAD SR instance contents. Subsequent changes to the displayed operating point are implementation dependent.

Prev | Up | Next
TID 4022 CAD Observation Context | Home | Chest CAD SR IOD Templates