C.4 Warning Status Class
Prev | C Status Type Encoding (Normative) | Next

## C.4 Warning Status Class

Statuses in this Status Class convey that the operation/notification has completed but an error was detected. The semantics and behavior of these Statuses are defined in PS3.4.

### C.4.1 Warning

Status Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Status | (0000,0900) | US | 1 | Confirmation status of the operation. The value of this required field is Service Class specific and defined in PS3.4.
Offending Element | (0000,0901) | AT | 1-n | This optional field contains a list of the elements in which the error was detected.
Error Comment | (0000,0902) | LO | 1 | This optional field contains an application-specific text description of the error detected.

Prev | Up | Next
C.3 Cancel Status Class | Home | C.4.2 Attribute List Error