A.77.4 Wide Field Ophthalmic Photography 3D Coordinates Image IOD Content Constraints
Prev | A.77 Wide Field Ophthalmic Photography 3D Coordinates Image Information Object Definition | Next

### A.77.4 Wide Field Ophthalmic Photography 3D Coordinates Image IOD Content Constraints

The following constraints on Series and Image attributes take precedence over the descriptions given in the Module Attribute Tables.

#### A.77.4.1 Bits Allocated, Bits Stored, and High Bit

These Attributes shall be determined based upon the Photometric Interpretation (0028,0004) :

Photometric Interpretation (0028,0004) | Bits Allocated (0028,0100) | Bits Stored (0028,0101) | High Bit (0028,0102)
--- | --- | --- | ---
MONOCHROME2 | 8 | 8 | 7
16 | 16 | 15
RGB YBR_FULL_422 YBR_PARTIAL_420 YBR_ICT YBR_RCT | 8 | 8 | 7

Prev | Up | Next
A.77.3 Wide Field Ophthalmic Photography 3D Coordinates Image IOD Modules | Home | A.77.4.2 Contrast/bolus Agent Sequence