F.4.2.3 STORAGE-SCP Application Entity Specification
Prev | F.4.2 AE Specifications | Next

#### F.4.2.3 STORAGE-SCP Application Entity Specification

##### F.4.2.3.1 SOP Classes

The STORAGE-SCP AE provides Standard Conformance to the following DICOM V3.0 SOP Classes:

Table F.4.2-22. SOP Classes for STORAGE-SCP AE

SOP Class Name | SOP Class UID | SCU | SCP
--- | --- | --- | ---
Verification | 1.2.840.10008.1.1 | Yes | Yes
Storage Commitment Push Model | 1.2.840.10008.1.20.1 | No | Yes
US Image Storage (Retired) | 1.2.840.10008.5.1.4.1.1.6 | No | Yes
US Image Storage | 1.2.840.10008.5.1.4.1.1.6.1 | No | Yes
US Multi-frame Storage (Retired) | 1.2.840.10008.5.1.4.1.1.3 | No | Yes
US Multi-frame Storage | 1.2.840.10008.5.1.4.1.1.3.1 | No | Yes
Computed Radiography Image Storage | 1.2.840.10008.5.1.4.1.1.1 | No | Yes
CT Image Storage | 1.2.840.10008.5.1.4.1.1.2 | No | Yes
MR Image Storage | 1.2.840.10008.5.1.4.1.1.4 | No | Yes
Secondary Capture Image Storage | 1.2.840.10008.5.1.4.1.1.7 | No | Yes

These are the default SOP Classes supported. By altering the configuration it is possible to support additional or fewer SOP Classes.

Prev | Up | Next
F.4.2.2.4 Association Acceptance Policy | Home | F.4.2.3.2 Association Policies