A.34.3.4.5 Number of Waveform Samples
Prev | A.34.3.4 12-Lead ECG IOD Content Constraints | Next

##### A.34.3.4.5 Number of Waveform Samples

The value of Number of Waveform Samples (003A,0010) in each Waveform Sequence Item shall be less than or equal to 16384.

### Note

This allows over 16 seconds per channel at the maximum sampling frequency; if longer recordings are required, the General ECG IOD may be used.

Prev | Up | Next
A.34.3.4.4 Number of Waveform Channels | Home | A.34.3.4.6 Sampling Frequency