6.3 WADO-URI Response
Prev | 6 Data Communication Requirements | Next

## 6.3 WADO-URI Response

The response shall be an HTTP Response Message as specified in IETF RFC7230.

### Note

The content of the message-body varies according to the Media type as defined below.

### 6.3.1 Body of Single DICOM MIME Sub-type Part Response

#### 6.3.1.1 MIME Type

The MIME type shall be 'application/dicom', as specified in IETF RFC3240.

#### 6.3.1.2 Content

The body content shall be a "Part 10 File" that includes a meta-header as defined in PS3.10.

#### 6.3.1.3 Transfer Syntax

The returned DICOM object shall be encoded using one of the transfer syntaxes specified in the transfer syntax query parameter as defined in Section 8.2.11 below. By default, the transfer syntax shall be "Explicit VR Little Endian".

### Note

This implies that retrieved images are sent uncompressed by default.

Prev | Up | Next
6.2.3 List of Character Sets Supported in the Response | Home | 6.3.2 Body of Non-DICOM MIME Type Response