6.9.11 SendEventReport
Prev | 6.9 UPS-RS Worklist Service | Next

### 6.9.11 SendEventReport

This operation sends an Event Report over an established WebSocket connection.

#### 6.9.11.1 Request

The request message shall be formed as follows:

- Resource

  - N/A

- Method

  - WebSocket Data Frame transmission

- The Event Report shall contain all mandatory attributes described indescribed in Table CC.2.4-1 in PS3.4 and Table 10.3-1 in PS3.7 for the event type.

##### 6.9.11.1.1 Request Message Body

WebSocket Events are encoded as WebSocket data frames with an opcode of "%x1" (text).

The frame payload data shall be a DICOM JSON dataset containing the attributes of the Event Report.

### Note

1. Example WebSocket payload:

       {
       "00000002": [ "1.2.840.10008.5.1.4.34.​6.​4" ],
       "00000100": [ 256 ],
       "00000110": [ 23 ],
       "00001000": [ "1.2.840.10008.5.1.4.34.​6.​4.2.3.44.22231" ],
       "00001001": [ 1 ],
       "00741238": [ "SCHEDULED" ],
       "00744041": [ "READY" ]
       }

2. The WebSocket protocol does not allow content negotiation so it is not possible to support both XML and JSON encoding of Event Report messages without extending the protocol.

Prev | Up | Next
6.9.10.3.2 Response Message Body | Home | 6.9.11.2 Behavior