F.2.7 InlineBinary
Prev | F.2 DICOM JSON Model | Next

### F.2.7 InlineBinary

If an attribute contains an "InlineBinary", this contains the base64 encoding of the enclosing attribute's Value Field.

There is a single InlineBinary value representing the entire Value Field, and not one per Value in the case where the Value Multiplicity is greater than one. E.g., a LUT with 4096 16 bit entries that may be encoded in DICOM with a Value Representation of OW, with a VL of 8192 and a VM of 1, or a US VR with a VL of 8192 and a VM of 4096 would both be represented as a single InlineBinary string.

All rules (e.g., byte ordering and swapping) in DICOM PS3.5 apply.

### Note

Implementers should in particular pay attention to the PS3.5 rules regarding the value representations of OD, OF and OW.

Prev | Up | Next
F.2.6 BulkDataURI | Home | F.3 Transformation with other DICOM Formats