TID 4122 CAD Common Image Properties Entry
Prev | Colon CAD SR IOD Templates | Next

### TID 4122 CAD Common Image Properties Entry

Each instance of the CAD Common Image Properties Entry Template contains selected attributes for a set of parallel contiguous equally spaced slices (with identical properties) from which CAD findings are derived.

Type:

  Extensible

Order:

  Significant

Root:

  No

Table TID 4122. CAD Common Image Properties Entry

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CONTAINER | EV (112224, DCM, "Image Set Properties") | 1 | M |  |
2 | > | CONTAINS | UIDREF | EV (112227, DCM, "Frame of Reference UID") | 1 | M |  |
3 | > | CONTAINS | UIDREF | EV (110180, DCM, "Study Instance UID") | 1 | M |  |
4 | > | CONTAINS | DATE | EV (111060, DCM, "Study Date") | 1 | M |  | Shall be taken from Study Date (0008,0020) in the Image Instances.
5 | > | CONTAINS | TIME | EV (111061, DCM, "Study Time") | 1 | M |  | Shall be taken from Study Time (0008,0030) in the Image Instances.
6 | > | CONTAINS | CODE | EV (121139, DCM, "Modality") | 1 | M |  | Shall be taken from Modality (0008,0060) in the Image Instances.
7 | > | CONTAINS | NUM | EV (111026, DCM, "Horizontal Pixel Spacing") | 1 | M |  | Shall be taken from value 1 of Pixel Spacing (0028,0030) in the Image Instances. UNITS = EV (mm/{pixel}, UCUM, "millimeters per pixel")
8 | > | CONTAINS | NUM | EV (111066, DCM, "Vertical Pixel Spacing") | 1 | M |  | Shall be taken from value 2 of Pixel Spacing (0028,0030) in the Image Instances. UNITS = EV (mm/{pixel}, UCUM, "millimeters per pixel")
9 | > | CONTAINS | NUM | EV (112225, DCM, "Slice Thickness") | 1 | M |  | Shall be taken from Slice Thickness (0018,0050) in the Image Instances. UNITS = EV (mm, UCUM, "millimeter")
10 | > | CONTAINS | NUM | EV (112226, DCM, "Spacing between slices") | 1 | M |  | Shall be computed from the Image Position (Patient) (0020,0032) projected onto the normal to the Image Orientation (Patient) (0020,0037); may or may not be the same as the Spacing Between Slices (0018,0088) if present. UNITS = EV (mm, UCUM, "millimeter")
11 | > | CONTAINS | CODE | EV (112228, DCM, "Recumbent Patient Position with respect to gravity") | 1 | MC | Required if Patient Position (0018,5100) is present in the image instances and has a value. | Shall be derived from Patient Position (0018,5100) in the Image Instances. DCID 6206 “Recumbent Patient Orientation for Colon”

Prev | Up | Next
TID 4121 Colon CAD Findings Summary | Home | TID 4125 Colon CAD Composite Feature