C.8.8.2.6 Image Pixel Module Attributes
Prev | C.8.8.2 RT Image Module | Next

##### C.8.8.2.6 Image Pixel Module Attributes

###### C.8.8.2.6.1 Samples Per Pixel

Enumerated Values:

1

###### C.8.8.2.6.2 Photometric Interpretation

Enumerated Values:

MONOCHROME2

###### C.8.8.2.6.3 Bits Allocated

Enumerated Values:

8

16

###### C.8.8.2.6.4 Bits Stored

Enumerated Values when Bits Allocated (0028,0100) is 8:

8

Enumerated Values when Bits Allocated (0028,0100) is 16:

12

13

14

15

16

###### C.8.8.2.6.5 High Bit

For RT Images, High Bit (0028,0102) shall be one less than the value sent in Bits Stored (0028,0101).

###### C.8.8.2.6.6 Pixel Representation

Enumerated Values when Bits Allocated (0028,0100) is 8:

0000H

  unsigned integer

Prev | Up | Next
C.8.8.2.5 Single-Frame and Multi-frame Images | Home | C.8.8.2.7 RT Image Plane, Position and Orientation