QQQ Parametric Maps (Informative)
Prev |  | Next

# QQQ Parametric Maps (Informative)

## QQQ.1

This Annex contains examples of the use of the Parametric Map IOD.

### QQQ.1.1

This Section contains an example of the use of the Parametric Map IOD to encode Ktrans for a Dynamic Contrast Enhanced (DCE) MR.

The frames comprise a single traversal of a regularly sampled 3D volume, described as a single stack and a single quantity, with dimensions of Stack ID, In-Stack Position Number and Quantity. A reference is also provided to the (single entire multi-frame) MR image from which the parametric map was derived. Only the Frame Content Sequence and Plane Position Sequence vary per-frame; all other functional groups are shared in this example.

Nesting | Attribute | Tag | VR | VL (hex) | Value
--- | --- | --- | --- | --- | ---
| Specific Character Set | (0008,0005) | CS | 000a | ISO_IR 100
| Image Type | (0008,0008) | CS | 0022 | DERIVED\SECONDARY\PERFUSION\KTRANS
| Instance Creation Date | (0008,0012) | DA | 0008 | 20140312
| Instance Creation Time | (0008,0013) | TM | 000a | 141900.944
| Instance Creator UID | (0008,0014) | UI | 0016 | 1.3.6.1.4.1.5962.99.3
| SOP Class UID | (0008,0016) | UI | 0016 | 1.3.6.1.4.1.5962.301.9
| SOP Instance UID | (0008,0018) | UI | 003e | 1.3.6.1.4.1.5962.99.1.3078904268.1788845519.1394648340940.2.0
| Study Date | (0008,0020) | DA | 0008 | 20140312
| Series Date | (0008,0021) | DA | 0008 | 20140312
| Content Date | (0008,0023) | DA | 0008 | 20140312
| Study Time | (0008,0030) | TM | 000a | 141900.944
| Series Time | (0008,0031) | TM | 000a | 141900.944
| Content Time | (0008,0033) | TM | 000a | 141900.944
| Accession Number | (0008,0050) | SH | 0000 |
| Modality | (0008,0060) | CS | 0002 | MR
| Manufacturer | (0008,0070) | LO | 0000 |
| Referring Physician's Name | (0008,0090) | PN | 0008 | Doe^John
| Study Description | (0008,1030) | LO | 002C | Dynamic magnetic resonance imaging of pelvis
| Procedure Code Sequence | (0008,1032) | SQ | ffffffff |
%item |  |  |  |  |
| Code Value | (0008,0100) | SH | 0008 | P5-70694
| Coding Scheme Designator | (0008,0102) | SH | 0004 | SRT
| Code Meaning | (0008,0104) | LO | 002C | Dynamic magnetic resonance imaging of pelvis
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Series Description | (0008,103E) | LO | 0010 | PK Model Results
| Patient's Name | (0010,0010) | PN | 0008 | Doe^Jane
| Patient ID | (0010,0020) | LO | 0004 | 1234
| Patient's Birth Date | (0010,0030) | DA | 0000 |
| Patient's Sex | (0010,0040) | CS | 0000 |
| Study Instance UID | (0020,000d) | UI | 003e | 1.3.6.1.4.1.5962.99.1.3078904268.1788845519.1394648340940.4.0
| Series Instance UID | (0020,000e) | UI | 003e | 1.3.6.1.4.1.5962.99.1.3078904268.1788845519.1394648340940.3.0
| Study ID | (0020,0010) | SH | 0004 | 5678
| Series Number | (0020,0011) | IS | 0004 | 100
| Instance Number | (0020,0013) | IS | 0002 | 1
| Patient Orientation | (0020,0020) | CS | 0000 |
| Frame of Reference UID | (0020,0052) | UI | 003e | 1.3.6.1.4.1.5962.99.1.3078904268.1788845519.1394648340940.5.0
| Position Reference Indicator | (0020,1040) | LO | 0000 |
| Dimension Organization Sequence | (0020,9221) | SQ | ffffffff |
%item |  |  |  |  |
| Dimension Organization UID | (0020,9164) | UI | 003e | 1.3.6.1.4.1.5962.99.1.3078904268.1788845519.1394648340940.6.0
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Dimension Index Sequence | (0020,9222) | SQ | ffffffff |
%item |  |  |  |  |
| Dimension Organization UID | (0020,9164) | UI | 003e | 1.3.6.1.4.1.5962.99.1.3078904268.1788845519.1394648340940.6.0
| Dimension Index Pointer | (0020,9165) | AT | 0004 | (0020,9056)
| Functional Group Pointer | (0020,9167) | AT | 0004 | (0040,9096)
| Dimension Description Label | (0020,9421) | LO | 0008 | Stack ID
%enditem |  |  |  |  |
%item |  |  |  |  |
| Dimension Organization UID | (0020,9164) | UI | 003e | 1.3.6.1.4.1.5962.99.1.3078904268.1788845519.1394648340940.6.0
| Dimension Index Pointer | (0020,9165) | AT | 0004 | (0020,9057)
| Functional Group Pointer | (0020,9167) | AT | 0004 | (0020,9111)
| Dimension Description Label | (0020,9421) | LO | 0018 | In-Stack Position Number
%enditem |  |  |  |  |
%item |  |  |  |  |
| Dimension Organization UID | (0020,9164) | UI | 003e | 1.3.6.1.4.1.5962.99.1.3078904268.1788845519.1394648340940.6.0
| Dimension Index Pointer | (0020,9165) | AT | 0004 | (0040,9220) (the Quantity Definition Code Sequence (CP 1387))
| Functional Group Pointer | (0020,9167) | AT | 0004 | (0020,9111)
| Dimension Description Label | (0020,9421) | LO | 0008 | Quantity
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Samples per Pixel | (0028,0002) | US | 0002 | 0001
| Photometric Interpretation | (0028,0004) | CS | 000c | MONOCHROME2
| Number of Frames | (0028,0008) | IS | 0002 | 14
| Rows | (0028,0010) | US | 0002 | 256 dec
| Columns | (0028,0011) | US | 0002 | 256 dec
| Bits Allocated | (0028,0100) | US | 0002 | 0020 hex
| Burned In Annotation | (0028,0301) | CS | 0002 | NO
| Recognizable Visual Features | (0028,0302) | CS | 0002 | NO
| Lossy Image Compression | (0028,2110) | CS | 0002 | 00
| Presentation LUT Shape | (2050,0020) | CS | 0008 | IDENTITY
| Shared Functional Groups Sequence | (5200,9229) | SQ | ffffffff |
%item |  |  |  |  |
| Derivation Image Sequence | (0008,9124) | SQ | ffffffff |
%item |  |  |  |  |
| Source Image Sequence | (0008,2112) | SQ | ffffffff |
%item |  |  |  |  |
| Referenced SOP Class UID | (0008,1150) | UI | 001C | 1.2.840.10008.5.1.4.1.1.4.1
| Referenced SOP Instance UID | (0008,1155) | UI | 002E | 1.3.6.1.4.1.5962.1.1.0.0.0.1410021852.13877.0
| Spatial Locations Preserved | (0028,135A) | CS | 0004 | YES
| Purpose of Reference Code Sequence | (0040,A170) | SQ | ffffffff |
%item |  |  |  |  |
| Code Value | (0008,0100) | SH | 0006 | 121322
| Coding Scheme Designator | (0008,0102) | SH | 0004 | DCM
| Code Meaning | (0008,0104) | LO | 002C | Source image for image processing operation
%enditem |  |  |  |  |
%endseq |  |  |  |  |
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Derivation Code Sequence | (0008,9215) | SQ | ffffffff |
%item |  |  |  |  |
| Code Value | (0008,0100) | SH | 0006 | 113066
| Coding Scheme Designator | (0008,0102) | SH | 0004 | DCM
| Code Meaning | (0008,0104) | LO | 000C | Time Course of Signal
%enditem |  |  |  |  |
%endseq |  |  |  |  |
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Frame Anatomy Sequence | (0020,9071) | SQ | ffffffff |
%item |  |  |  |  |
| Anatomic Region Sequence | (0008,2218) | SQ | ffffffff |
%item |  |  |  |  |
| Code Value | (0008,0100) | SH | 0008 | T-9200B
| Coding Scheme Designator | (0008,0102) | SH | 0004 | SRT
| Code Meaning | (0008,0104) | LO | 0008 | Prostate
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Frame Laterality | (0020,9072) | CS | 0002 | U
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Plane Orientation Sequence | (0020,9116) | SQ | ffffffff |
%item |  |  |  |  |
| Image Orientation (Patient) | (0020,0037) | DS | 0064 | 0.99979773312597\​-.0160528955995\​.012115996823878\​.012116000683426\​0.96149705857037\​.274548008348208
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Pixel Measures Sequence | (0028,9110) | SQ | ffffffff |
%item |  |  |  |  |
| Slice Thickness | (0018,0050) | DS | 0010 | 5.9999942779541
| Pixel Spacing | (0028,0030) | DS | 0022 | 1.01559996604919\1.01560020446777
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Frame VOI LUT Sequence | (0028,9132) | SQ | ffffffff |
%item |  |  |  |  |
| Window Center | (0028,1050) | DS | 0004 | 2.5
| Window Width | (0028,1051) | DS | 0002 | 5
| VOI LUT Function | (0028,1056) | CS | 000c | LINEAR_EXACT
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Pixel Value Transformation Sequence | (0028,9145) | SQ | ffffffff |
%item |  |  |  |  |
| Rescale Intercept | (0028,1052) | DS | 0002 | 0
| Rescale Slope | (0028,1053) | DS | 0002 | 1
| Rescale Type | (0028,1054) | LO | 0002 | US
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Real World Value Mapping Sequence | (0040,9096) | SQ | ffffffff |
%item |  |  |  |  |
| LUT Explanation | (0028,3003) | LO | 0006 | Ktrans
| Measurement Units Code Sequence | (0040,08ea) | SQ | ffffffff |
%item |  |  |  |  |
| Code Value | (0008,0100) | SH | 0004 | /min
| Coding Scheme Designator | (0008,0102) | SH | 0004 | UCUM
| Code Meaning | (0008,0104) | LO | 0004 | /min
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| LUT Label | (0040,9210) | SH | 0006 | Ktrans
| Real World Value Last Value Mapped | (0040,9211) | XS | 0002 | 0005
| Real World Value First Value Mapped | (0040,9216) | XS | 0002 | 0000
| Real World Value Intercept | (0040,9224) | FD | 0008 | 0
| Real World Value Slope | (0040,9225) | FD | 0008 | 1
| Quantity Definition Code Sequence (CP 1387) | (0040,9220) | SQ | ffffffff |
%item |  |  |  |  |
| Value Type | (0040,a040) | CS | 0004 | CODE
| Concept Name Code Sequence | (0040,a043) | SQ | ffffffff |
%item |  |  |  |  |
| Code Value | (0008,0100) | SH | 0006 | G-C1C6
| Coding Scheme Designator | (0008,0102) | SH | 0004 | SRT
| Code Meaning | (0008,0104) | LO | 0008 | Quantity
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Concept Code Sequence | (0040,a168) | SQ | ffffffff |
%item |  |  |  |  |
| Code Value | (0008,0100) | SH | 0006 | 126312
| Coding Scheme Designator | (0008,0102) | SH | 0004 | DCM
| Code Meaning | (0008,0104) | LO | 0006 | Ktrans
%enditem |  |  |  |  |
%endseq |  |  |  |  |
%enditem |  |  |  |  |
%item |  |  |  |  |
| Value Type | (0040,a040) | CS | 0004 | CODE
| Concept Name Code Sequence | (0040,a043) | SQ | ffffffff |
%item |  |  |  |  |
| Code Value | (0008,0100) | SH | 0006 | G-C036
| Coding Scheme Designator | (0008,0102) | SH | 0004 | SRT
| Code Meaning | (0008,0104) | LO | 0012 | Measurement Method
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Concept Code Sequence | (0040,a168) | SQ | ffffffff |
%item |  |  |  |  |
| Code Value | (0008,0100) | SH | 0006 | 126340
| Coding Scheme Designator | (0008,0102) | SH | 0004 | DCM
| Code Meaning | (0008,0104) | LO | 0014 | Standard Tofts Model
%enditem |  |  |  |  |
%endseq |  |  |  |  |
%enditem |  |  |  |  |
%endseq |  |  |  |  |
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Parametric Map Frame Type Sequence | (0040,9092) | SQ | ffffffff |
%item |  |  |  |  |
| Frame Type | (0008,9007) | CS | 0022 | DERIVED\SECONDARY\PERFUSION\KTRANS
%enditem |  |  |  |  |
%endseq |  |  |  |  |
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Per-frame Functional Groups Sequence | (5200,9230) | SQ | ffffffff |
%item |  |  |  |  |
| Frame Content Sequence | (0020,9111) | SQ | ffffffff |
%item |  |  |  |  |
| Stack ID | (0020,9056) | SH | 0002 | 1
| In-Stack Position Number | (0020,9057) | UL | 0004 | 0001
| Dimension Index Values | (0020,9157) | UL | 000C | 00000001,00000001,00000001
%enditem |  |  |  |  |
%endseq |  |  |  |  |
| Plane Position Sequence | (0020,9113) | SQ | ffffffff |
%item |  |  |  |  |
| Image Position (Patient) | (0020,0032) | DS | 0032 | -153.28300476074\-111.93399810791\-54.366100311279
%enditem |  |  |  |  |
%endseq |  |  |  |  |
%enditem |  |  |  |  |
% | ... |  |  |  |
%endseq |  |  |  |  |
| Float Pixel Data | (7FE0,0008) | OF | 380000 | []

Prev |  | Next
PPP.3.2 An Example of A Tablet Display | Home | RRR Measurement Report SR Document for Planar and Volumetric ROI (Informative)