DICOM PS3.18 2016a - Web Services

8.2 Parameters for DICOM Image Persistent Objects
Prev | 8 Parameters of the Request | Next

## 8.2 Parameters for DICOM Image Persistent Objects

These parameters shall only be included when a request is made for a Single Frame Image Objects or Multi-Frame Image or video Objects as defined in Section 6.1.1.2.

Prev | Up | Next
8 Parameters of the Request | Home | 8.2.1 Annotation On The Object

DICOM PS3.18 2016a - Web Services