DICOM PS3.3 2016a - Information Object Definitions

A.34.3.4.8 Waveform Sample Interpretation
Prev | A.34.3.4 12-Lead ECG IOD Content Constraints | Next

##### A.34.3.4.8 Waveform Sample Interpretation

The value of Waveform Sample Interpretation (5400,1006) in each Waveform Sequence Item shall be SS.

Prev | Up | Next
A.34.3.4.7 Channel Source | Home | A.34.3.4.9 Waveform Annotation Module

DICOM PS3.3 2016a - Information Object Definitions