DICOM PS3.7 2016a - Message Exchange

10.3.6 N-DELETE Protocol
Prev | 10.3 Protocol | Next

### 10.3.6 N-DELETE Protocol

The information necessary for the N-DELETE request and indication DIMSE-N primitives are conveyed in the N-DELETE-RQ Message. The information necessary for the N-DELETE response and confirmation DIMSE-N primitives are conveyed in the N-DELETE-RSP Message.

#### 10.3.6.1 N-DELETE-RQ

The N-DELETE-RQ Message contains fields as defined in Table 10.3-11. Each field shall conform to DICOM encoding and Value Representation as defined in PS3.5. Fields are required as specified in the N-DELETE service definition unless otherwise noted in Table 10.3-11. Fields not specified in the N-DELETE service definition but present in Table 10.3-11 are required by the DIMSE-N protocol.

Table 10.3-11. N-DELETE-RQ Message Fields

Message Field | Tag | VR | VM | Description of Field
--- | --- | --- | --- | ---
Command Group Length | (0000,0000) | UL | 1 | The even number of bytes from the end of the value field to the beginning of the next group.
Requested SOP Class UID | (0000,0003) | UI | 1 | SOP Class UID of the SOP Instance to be deleted.
Command Field | (0000,0100) | US | 1 | This field distinguishes the DIMSE-N operation conveyed by this Message. The value of this field shall be set to 0150H for the N-DELETE-RQ Message.
Message ID | (0000,0110) | US | 1 | Implementation-specific value that distinguishes this Message from other Messages.
Command Data Set Type | (0000,0800) | US | 1 | This field indicates that no Data Set is present in the Message. It shall be set to the value of 0101H.
Requested SOP Instance UID | (0000,1001) | UI | 1 | Contains the UID of the SOP Instance to be deleted.

Prev | Up | Next
10.3.5.3 N-CREATE Protocol Procedures | Home | 10.3.6.2 N-DELETE-RSP

DICOM PS3.7 2016a - Message Exchange