DICOM PS3.3 2016a - Information Object Definitions

A.16.2 XRF Image IOD Entity-Relationship Model
Prev | A.16 X-Ray RF Image IOD | Next

### A.16.2 XRF Image IOD Entity-Relationship Model

The E-R Model in Section A.1.2 depicts those components of the DICOM Application Information Model that directly reference the X-Ray RF Image IOD, with exception of the Frame of Reference entity that is not used. Additionally, "Image" in Figure A.1-1 may represent a single-frame or a multi-frame image. A frame denotes a two-dimensional organization of pixels recorded as a single exposure.

### Note

When a Study (or Study Component) contains a number of Multi-frame images that do not need to be grouped under different Series, a single Series may be used with a series number containing an arbitrary value (e.g., 1).

Prev | Up | Next
A.16 X-Ray RF Image IOD | Home | A.16.3 XRF Image IOD Module Table

DICOM PS3.3 2016a - Information Object Definitions