DICOM PS3.3 2016b - Information Object Definitions

A.56.4 Enhanced PET Image Functional Group Macros
Prev | A.56 Enhanced PET Image IOD | Next

### A.56.4 Enhanced PET Image Functional Group Macros

Table A.56-2 specifies the use of the Functional Group Macros used in the Multi-frame Functional Groups Module for the Enhanced PET Image IOD.

Table A.56-2. Enhanced PET Image Functional Group Macros

Functional Group Macro | Section | Usage
--- | --- | ---
Pixel Measures | C.7.6.16.2.1 | M
Frame Content | C.7.6.16.2.2 | M - May not be used as a Shared Functional Group.
Plane Position (Patient) | C.7.6.16.2.3 | M
Plane Orientation (Patient) | C.7.6.16.2.4 | M
Referenced Image | C.7.6.16.2.5 | C - Required if the image or frame has been planned on another image or frame, may be present otherwise.
Derivation Image | C.7.6.16.2.6 | C - Required if the image or frame has been derived from another SOP Instance.
Frame Anatomy | C.7.6.16.2.8 | M
Pixel Value Transformation | C.7.6.16.2.9 | M
Frame VOI LUT | C.7.6.16.2.10 | M
Real World Value Mapping | C.7.6.16.2.11 | M - The Defined CID for Measurement Units Code Sequence shall be CID 84 “PET Units”.
Cardiac Synchronization | C.7.6.16.2.7 | C - Required if Cardiac Synchronization Technique (0018,9037) equals other than NONE. May be present otherwise.
Respiratory Synchronization | C.7.6.16.2.17 | C - Required if Respiratory Motion Compensation Technique (0018,9170) equals other than NONE. May be present otherwise.
Radiopharmaceutical Usage | C.7.6.16.2.19 | M
Patient Physiological State | C.7.6.16.2.20 | C - Required for cardiac rest and stress images.
PET Frame Type | C.8.22.5.1 | M
PET Frame Acquisition | C.8.22.5.2 | C - Required if Image Type (0008,0008) Value 1 equals ORIGINAL. May be present otherwise.
PET Detector Motion Details | C.8.22.5.3 | C - Required if Image Type (0008,0008) Value 1 equals ORIGINAL and Type of Detector Motion (0054,0202) is not equal to STATIONARY.
PET Position | C.8.22.5.4 | C - Required if Image Type (0008,0008) Value 1 equals ORIGINAL. May be present otherwise.
PET Frame Correction Factors | C.8.22.5.5 | C - Required if Image Type (0008,0008) Value 1 equals ORIGINAL. May be present otherwise.
PET Reconstruction | C.8.22.5.6 | C - Required if Image Type (0008,0008) Value 1 equals ORIGINAL. May be present otherwise.
PET Table Dynamics | C.8.22.5.7 | C - Required if Image Type (0008,0008) Value 1 equals ORIGINAL and Table Motion (0018,1134) is equal to DYNAMIC.

Prev | Up | Next
A.56.3 Enhanced PET Image IOD Module Table | Home | A.56.5 Acquisition Context Module

DICOM PS3.3 2016b - Information Object Definitions