DICOM PS3.16 2016b - Content Mapping Resource

CID 3227 QTc Measurements
Prev | B DCMR Context Groups (Normative) | Next

## CID 3227 QTc Measurements

This Context Group include both global and per lead corrected QT measurements specified in the ISO/IEEE 11073-10102 MDC nomenclature. Note that the MDC code for the per lead measurement is a base code for post-coordination with separately encoded lead identifiers. MDC also defines pre-coordinated codes that include both the measurement and the lead, which may be used in the same context as this Context Group; see the ISO/IEEE Standard.

While this Context Group includes distinct codes for the various QT correction algorithms, Templates using this Context Group may allow post-coordination using the QTc algorithm codes of CID 3678 “QT Correction Algorithms”.

### Note

Codes reprinted by permission of IEEE, Copyright 2004 by IEEE. ISO/IEEE 11073-10102 available through http://standards.ieee.org/.

Type:

  Extensible

Version:

  20110330

Table CID 3227. QTc Measurements

Coding Scheme Designator | Code Value | Code Meaning | ISO/IEEE 11073 MDC Equivalent Reference ID (Informative)
--- | --- | --- | ---
MDC | 2:15876 | QTc interval global | MDC_ECG_TIME_PD_QTC
MDC | 2: 33792 | QTc interval per lead | MDC_ECG_TIME_PD_QTC_<lead>
MDC | 2:15880 | QTc global using Bazett formula | MDC_ECG_TIME_PD_QTC_BAZETT
MDC | 2:15880 | QTc global using Framingham formula | MDC_ECG_TIME_PD_QTC_FRAMINGHAM
MDC | 2:15892 | QTc global using Fredericia formula | MDC_ECG_TIME_PD_QTC_FREDERICA
MDC | 2:15892 | QTc global using Hodges formula | MDC_ECG_TIME_PD_QTC_HODGES
MDC | 2:34048 | QTc per lead using Bazett formula | MDC_ECG_TIME_PD_QTcB_<lead>
MDC | 2:34304 | QTc per lead using Fredericia formula | MDC_ECG_TIME_PD_QTcF_<lead>

Prev | Up | Next
CID 3221 Stress Test Termination Reasons | Home | CID 3228 ECG Timing Measurements

DICOM PS3.16 2016b - Content Mapping Resource