DICOM PS3.3 2016b - Information Object Definitions

A.34.10.4.6 Waveform Sample Interpretation
Prev | A.34.10.4 General Audio Waveform IOD Content Constraints | Next

##### A.34.10.4.6 Waveform Sample Interpretation

The value of Waveform Sample Interpretation (5400,1006) in each Waveform Sequence Item shall be SB or SS.

Prev | Up | Next
A.34.10.4.5 Channel Source | Home | A.35 Structured Report Document Information Object Definitions

DICOM PS3.3 2016b - Information Object Definitions