DICOM PS3.4 2016b - Service Class Specifications

T.4.4.2 SCP Conformance Requirements
Prev | T.4.4 Conformance Statement Requirements | Next

#### T.4.4.2 SCP Conformance Requirements

An implementation that conforms to the Hanging Protocol Storage SOP Class as an SCP that interprets Hanging Protocol SOP Instances for display shall state in its Conformance Statement:

- The range of display environments that the SCP will support (e.g., number of screens, size of screens, overlapping image boxes).

- The optional Attributes of the Hanging Protocol IOD that it is capable of interpreting and those that are not supported.

- Description of application behavior when the value of Partial Data Display Handling (0072,0208) is ADAPT_LAYOUT or zero length.

- Description of application behavior when the display environment of the Hanging Protocol Instance differs from the display environment of the application, with respect to preserving layout versus spatial resolution.

- The Image Storage SOP Classes for which the Hanging Protocol Storage SOP Class is supported

An implementation that conforms to the Hanging Protocol Storage SOP Class as an SCP shall state in its Conformance Statement:

- The behavior of the SCP in the case of a successful C-STORE operation, including the access method for a stored Hanging Protocol SOP Instance, and the duration of the storage.

- The meaning of each case of a failure C-STORE response status, as well as appropriate recovery action.

Prev | Up | Next
T.4.4 Conformance Statement Requirements | Home | U Hanging Protocol Query/Retrieve Service Class

DICOM PS3.4 2016b - Service Class Specifications