DICOM PS3.16 2016b - Content Mapping Resource

TID 4004 Mammography CAD Composite Feature
Prev | Mammography CAD SR IOD Templates | Next

### TID 4004 Mammography CAD Composite Feature

This Template collects a composite feature for a lesion, non-lesion object, or correlation of related objects. The details of the composition are expressed in the Mammography CAD Composite Feature Body (see TID 4005 “Mammography CAD Composite Feature Body”). The data from which the details are inferred, are expressed in the Composite Features (see TID 4004 “Mammography CAD Composite Feature”) and/or Single Image Findings (see TID 4006 “Mammography CAD Single Image Finding”), of which there may be several.

A Composite Feature shall be INFERRED FROM any combination of two or more Composite Features or Single Image Findings or mixture thereof.

Type:

  Non-Extensible

Order:

  Significant

Root:

  No

Table TID 4004. Mammography CAD Composite Feature

| NL | Rel with Parent | VT | Concept Name | VM | Req Type | Condition | Value Set Constraint
--- | --- | --- | --- | --- | --- | --- | --- | ---
1 |  |  | CODE | EV (111015, DCM, "Composite Feature") | 1 | M |  | DCID 6016 “Mammography Composite Feature”
2 | > | HAS CONCEPT MOD | CODE | EV (111056, DCM, "Rendering Intent") | 1 | M |  | DCID 6034 “Intended Use of CAD Output”
3 | > | HAS OBS CONTEXT | INCLUDE | DTID 4108 “Tracking Identifier” | 1 | U |  |
4 | > | HAS PROPERTIES | INCLUDE | DTID 4005 “Mammography CAD Composite Feature Body” | 1 | M |  |
5 | > | INFERRED FROM | INCLUDE | DTID 4004 “Mammography CAD Composite Feature” | 1-n | MC | At least two items shall be present: two of row 5, two of row 6, or one of each. |
6 | > | INFERRED FROM | INCLUDE | DTID 4006 “Mammography CAD Single Image Finding” | 1-n | MC | At least two items shall be present: two of row 5, two of row 6, or one of each. |
7 | > | HAS OBS CONTEXT | INCLUDE | DTID 4022 “CAD Observation Context” | 1 | MC | Shall be present only if this feature is incorporated from a different report than its parent. |

Content Item Descriptions

Rendering Intent | This Content Item constrains the SCP receiving the Mammography CAD SR IOD in its use of the contents of this Template and its Target Content Items. Mammography CAD devices may opt to use data marked "Not for Presentation" or "Presentation Optional" as input to subsequent mammography CAD processing steps. Refer to Section O.2 “Structured Reporting Storage SOP Class SCU and SCP Behavior” in PS3.4 .

Prev | Up | Next
TID 4003 Mammography CAD Individual Impression/Recommendation | Home | TID 4005 Mammography CAD Composite Feature Body

DICOM PS3.16 2016b - Content Mapping Resource